{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","47"]
["","Ψύξη","","Ονομ.","dBA","46"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1"]
["","Βιδωτή σακούλα","","","","1"]
["","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","","","","1"]
["","Πώμα αποχέτευσης (1)","","","","6"]
["","Πώμα αποχέτευσης (2)","","","","3"]
["","Αφαιρούμενη ετικέτα αερίου F","","","","1"]
["","Ετικέτα πρόσθετου φορτίου ψυκτικού","","","","1"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Φορτίο","","","kg","1.8"]
["","Τύπος","","","","R-32"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","σ.α.λ.","420"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","σ.α.λ.","420"]
["Συνδέσεις σωληνώσεων","Υψομετρική διαφορά","ΕΣ.-ΕΣ.","Μέγ.","m","7.5"]
["","","ΕΣ.-ΕΞ.","Μέγ.","m","15"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)"]
["","Συνολικό μήκος σωληνώσεων","Σύστημα","Πραγματικό","m","50"]
["Συμπιεστής","Type","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Πλάτος","χιλ.","868"]
["","","","Βάθος","χιλ.","320"]
["","","","Ύψος","χιλ.","734"]
["Βάρος","Μονάδα","","","kg","57"]
["Power supply","Phase","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","220-240"]
["Σημειώσεις","","","","","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["","","","","","(2) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Εξαιρετικά χαμηλές","m³/min","","24"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","m³/min","","24"]
["","","","Εξαιρετικά χαμηλές","cfm","","847"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","cfm","","847"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","","734"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","","868"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","","320"]
["Βάρος","Μονάδα","","","kg","","57"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Ψύξη-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","σ.α.λ.","","420"]
["","","Θέρμανση","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Θέρμανση-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","σ.α.λ.","","420"]
["Συμπιεστής","Type","","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","","-10"]
["","","","Μέγ.","°CDB","","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","","-15"]
["","","","Μέγ.","°CWB","","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","","46"]
["","Θέρμανση","","Ονομ.","dBA","","47"]
["Ψυκτικό μέσο","Τύπος","","","","","R-32"]
["","Φορτίο","","","kg","","1.80"]
["","Φορτίο","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","","25"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","15"]
["","","ΕΣ.-ΕΣ.","Μέγ.","m","","7.5"]
["","Συνολικό μήκος σωληνώσεων","Σύστημα","Πραγματικό","m","","50"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Τροφοδοσία ισχύος","Φάση","","","","","1~"]
["","Συχνότητα","","","Hz","","50"]
["","Τάση","","","V","","220-240"]