{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-A8"]
[]
[]
[]
[]
["","","","","","4MXM68A2V1B8","4MXM80A2V1B8"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","734","734"]
["","","","Πλάτος","mm","974","974"]
["","","","Βάθος","mm","408","408"]
["Βάρος","Μονάδα","","","kg","63","67"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10"]
["","","","Μέγ.","°CDB","50","50"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","48","48"]
["","Θέρμανση","","Ονομ.","dBA","49","49"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32"]
["","Φορτίο","","","kg","2.00","2.40"]
["","Φορτίο","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","25 (1)","25 (1)"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15","15"]
["","","ΕΣ.-ΕΣ.","Μέγ.","m","7.5","7.5"]
["","Συνολικό μήκος σωληνώσεων","Σύστημα","Πραγματικό","m","60","70"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","A+++ ~ D","A+++ ~ D"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]
["Σημειώσεις","","","","","(1) - Για ένα δωμάτιο","(1) - Για ένα δωμάτιο"]
["","","","","","(2) - Για συνδυασμό με CVXM-A, FVXM-A - το μέγιστο μήκος σωληνώσεων είναι 30 μ.","(2) - Για συνδυασμό με CVXM-A, FVXM-A - το μέγιστο μήκος σωληνώσεων είναι 30 μ."]
["","","","","","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","","(5) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(5) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]