{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","","44","","47"]
["","","","Ονομ.","dBA","","41","","44"]
["","","","Αθόρυβη λειτουργία","dBA","","36","","41"]
["","","","Χαμηλή","dBA","","38","","43"]
["","Ψύξη","","Αθόρυβη λειτουργία","dBA","","36","","41"]
["","","","Χαμηλή","dBA","","38","","43"]
["","","","Υψ.","dBA","","44","","47"]
["","","","Ονομ.","dBA","","41","","44"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","","Εγχειρίδιο εγκατάστασης","","Εγχειρίδιο εγκατάστασης"]
["","Εγχειρίδιο χειρισμού","","","","","Εγχειρίδιο χειρισμού","","Εγχειρίδιο χειρισμού"]
["","Κοχλίες","","","","","Κοχλίες","","Κοχλίες"]
["","Ροδέλα","","","","","Ροδέλα","","Ροδέλα"]
["","Ασύρματο τηλεχειριστήριο","","","","","Ασύρματο τηλεχειριστήριο","","Ασύρματο τηλεχειριστήριο"]
["","Σχάρα κλειδώματος καλύμματος","","","","","Σχάρα κλειδώματος καλύμματος","","Σχάρα κλειδώματος καλύμματος"]
["","Μπαταρία","","","","","Μπαταρία","","Μπαταρία"]
["Control systems","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","","9.52","","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","","15.88","","15.88"]
["","Drain","","","","","19.05","","19.05"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","0.094","","0.137"]
["","Θέρμανση","","Ονομ.","kW","","0.094","","0.137"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","56","","60"]
["","Θέρμανση","","","dBA","","56","","60"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","820","","820"]
["","","","Βάθος","mm","","820","","820"]
["","","","Ύψος","mm","","300","","300"]
["Casing","Material","","","","","Γαλβανισμένος χάλυβας","","Γαλβανισμένος χάλυβας"]
["Βάρος","Μονάδα","","","kg","","39","","39"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","","29.2","","34.0"]
["","","","Χαμηλή","m³/min","","21.0","","26.3"]
["","","","Ονομ.","m³/min","","24.4","","29.2"]
["","","Ψύξη","Χαμηλή","m³/min","","21.0","","26.3"]
["","","","Ονομ.","m³/min","","24.4","","29.2"]
["","","","Υψ.","m³/min","","29.2","","34.0"]
["","","","Αθόρυβη λειτουργία","m³/min","","17.6","","22.1"]
["","","Ψύξη","Αθόρυβη λειτουργία","m³/min","","17.6","","22.1"]
["Διακοσμητική μάσκα","Βάρος","","","kg","","4","","4"]
["","Διαστάσεις","","Ύψος","mm","","82","","82"]
["","","","Βάθος","mm","","990","","990"]
["","","","Πλάτος","mm","","990","","990"]
["","Χρώμα","","","","","Λευκό","","Λευκό"]
["Power supply","Φάση","","","","","1~","","1~"]
["","Όνομα","","","","","V1","","V1"]
["","Συχνότητα","","","Hz","","50","","50"]
["","Τάση","","","V","","220-240","","220-240"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Αθόρυβη λειτουργία","m³/min","15","","22.1"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","0.067","","0.137"]
["","Ψύξη","","Ονομ.","kW","0.067","","0.137"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Αθόρυβη λειτουργία","m³/min","15","","22.1"]
["Περίβλημα","Υλικό","","","","Γαλβανισμένος χάλυβας","","Γαλβανισμένος χάλυβας"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","265","","300"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","820","","820"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","820","","820"]
["Βάρος","Μονάδα","","","kg","31","","39"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","24.4","","34"]
["","","","Ονομ.","m³/min","20.5","","29.2"]
["","","","Χαμηλή","m³/min","17.6","","26.3"]
["","","Θέρμανση","Υψ.","m³/min","24.4","","34"]
["","","","Ονομ.","m³/min","20.5","","29.2"]
["","","","Χαμηλή","m³/min","17.6","","26.3"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","54","","60"]
["","Θέρμανση","","","dBA","54","","60"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","41","","47"]
["","","","Ονομ.","dBA","38","","44"]
["","","","Χαμηλή","dBA","35","","43"]
["","","","Αθόρυβη λειτουργία","dBA","32","","41"]
["","Θέρμανση","","Υψ.","dBA","41","","47"]
["","","","Ονομ.","dBA","38","","44"]
["","","","Χαμηλή","dBA","35","","43"]
["","","","Αθόρυβη λειτουργία","dBA","32","","41"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.52","","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","15.88","","15.88"]
["","Αποχέτευση","","","","19.05","","19.05"]
["Διακοσμητική μάσκα","Διαστάσεις","","Διακοσμητική μάσκα-=-Διαστάσεις-=-Ύψος-=-χιλ.","mm","82","","82"]
["","","","Διακοσμητική μάσκα-=-Διαστάσεις-=-Πλάτος-=-χιλ.","mm","990","","990"]
["","","","Διακοσμητική μάσκα-=-Διαστάσεις-=-Βάθος-=-χιλ.","mm","990","","990"]
["","Βάρος","","","kg","4","","4"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","ARCWLA","","ARCWLA"]
["","Τηλεχειριστήριο με καλώδιο","","","","ARCWB","","ARCWB"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","","1~"]
["","Συχνότητα","","","Hz","50","","50"]
["","Τάση","","","V","220-240","","220-240"]