{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / ARXS-L3"]
[]
[]
[]
[]
["","","","ADEQ35C2VEB / ARXS35L3V1B"]
["Απόδοση ψύξης","Ονομ.","kW","3.40 (1)"]
["Απόδοση σε λειτουργία θέρμανσης","Ονομ.","kW","4.00 (1)"]
["Σημειώσεις","","","(1) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]
["","","","(2) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","(3) - PED: συγκρότημα = κατηγορία Ι: εξαιρείται από το πλαίσιο της PED (Οδηγία για συσκευές πίεσης) λόγω του άρθρου 1, στοιχείο 3.6 της 97/23/EC"]
["","","","(4) - Ελάχιστη τιμή Ssc (=Ισχύς βραχυκυκλώματος): Εξοπλισμός που συμμορφώνεται με το πρότυπο EN 61000-3-2"]
["","","","(5) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","(6) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]