{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","0.106","0.149"]
["","Ψύξη","","Ονομ.","kW","0.106","0.149"]
["Ανεμιστήρας","Εξωτερική στατική πίεση","","Υψηλή","Pa","0","0","0","0"]
["","","","Χαμηλή","Pa","0","0","0","0"]
["Απόδοση ψύξης","Συνολική απόδοση","","Ονομ.","kW","","","12.10","13.00"]
["Απόδοση σε λειτουργία θέρμανσης","Συνολική απόδοση","","Ονομ.","kW","","","13.5","15.5"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό","Λευκό"]
["","Υλικό","","","","Γαλβανισμένος χάλυβας","Γαλβανισμένος χάλυβας"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","260","260","260","285"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","1320","1538","1790","1900"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","634","634","634","680"]
["Βάρος","Μονάδα","","","kg","38","45","65","70"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","23.8","31.1","34.4","43.9"]
["","","","Ονομ.","m³/min","21.3","27.8","31","39"]
["","","","Μέτρια","m³/min","","","31","39"]
["","","","Χαμηλή","m³/min","18.9","24.8","27.2","28.3"]
["","","Θέρμανση","Υψ.","m³/min","23.8","31.1","34.4","43.9"]
["","","","Ονομ.","m³/min","21.3","27.8","30.6","39.1"]
["","","","Μέτρια","m³/min","","","30.6","39.1"]
["","","","Χαμηλή","m³/min","18.9","24.8","27.2","28.3"]
["","Εξωτερική στατική πίεση","","Ονομ.","Pa","0","0","0","0"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","59","64","65","71"]
["","Θέρμανση","","","dBA","62","64","65","71"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","49","52","52","56"]
["","","","Ονομ.","dBA","48","47"]
["","","","Μέτρια","dBA","","","50","53"]
["","","","Χαμηλή","dBA","46","46","49","46"]
["","Θέρμανση","","Υψ.","dBA","49","52","52","56"]
["","","","Μέτρια","dBA","","","50","53"]
["","","","Ονομ.","dBA","48","47"]
["","","","Χαμηλή","dBA","46","46","49","46"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","9.52","9.52","9.52","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","15.88","15.88","15.9","15.9"]
["","Αποχέτευση","","","","19.05","19.05"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Τηλεχειριστήριο με καλώδιο","","","","ARCWB","ARCWB"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Σωλήνας αποχέτευσης","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]