{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":11,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARX-K"]
[]
[]
[]
[]
["","","","","","ARX20K2V1B","ARX20K5V1B9","ARX25K2V1B","ARX25K5V1B9","ARX35K2V1B","ARX35K5V1B9"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","550","550","550","550","550","550"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","658","658","658","658","658","658"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","275","275","275","275","275","275"]
["Βάρος","Μονάδα","","","kg","28","26","28","26","28","28"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)"]
["","","","Μέγ.","°CDB","46","46","46","46","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15","-15","-15","-15","-15","-15"]
["","","","Μέγ.","°CWB","18","18","18","18","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","46","46","46","46","48","48"]
["","Θέρμανση","","Υψ.","dBA","47","47","47","47","48","48"]
["Ψυκτικό μέσο","Τύπος","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Φορτίο","","","kg","0.74","0.74","0.74","0.74","1.0","1.0"]
["","Φορτίο","","","tCO2Eq","1.5","1.5","1.5","1.5","2.1","2.1"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","15","15","15","15","15","15"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","12","12","12","12","12","12"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - Εύρος λειτ. σε συνδ. με ΑTX-J3: ελάχ. 10°CDB ~ μέγ. 46°CDB","(1) - Εύρος λειτ. σε συνδ. με ΑTX-J3: ελάχ. 10°CDB ~ μέγ. 46°CDB","(1) - Εύρος λειτ. σε συνδ. με ΑTX-J3: ελάχ. 10°CDB ~ μέγ. 46°CDB","(1) - Εύρος λειτ. σε συνδ. με ΑTX-J3: ελάχ. 10°CDB ~ μέγ. 46°CDB","(1) - Εύρος λειτ. σε συνδ. με ΑTX-J3: ελάχ. 10°CDB ~ μέγ. 46°CDB","(1) - Εύρος λειτ. σε συνδ. με ΑTX-J3: ελάχ. 10°CDB ~ μέγ. 46°CDB"]
["Στάνταρτ εξαρτήματα","LOT10 Energy Label","","","","","LOT10 Energy Label","","LOT10 Energy Label","","LOT10 Energy Label"]