{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":13,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B","ARXM35R5V1B","ARXM50R2V1B","ARXM50R5V1B","ARXM60R5V1B","ARXM60R2V1B","ARXM71R2V1B","ARXM71R5V1B"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","550","550","734","734","734","734","734"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","765","765","954","954","954","954","954"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","285","285","401","401","401","401","401"]
["Βάρος","Μονάδα","","","kg","32","32","49.0","49.0","49.0","49.0","49.0","49.0"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10","-10","-10 (4) (5), -10 (4) (5)","-10","-10","-10","-10"]
["","","","Μέγ.","°CDB","50, 46","50, 46","50, 46","50 (4), 46 (5)","46","46","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15","-15","-15"]
["","","","Μέγ.","°CWB","18","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","46","49","48.0","48.0","48.0","48.0","52.0","52.0"]
["","Θέρμανση","","Ονομ.","dBA","47","49","49.0","49.0","49.0","49.0","52.0","52.0"]
["Ψυκτικό μέσο","Τύπος","","","","","","","","","","","R-32"]
["","Φορτίο","","","kg","0.76","0.76","1.15","1.15","1.15","1.15","1.15","1.15"]
["","Φορτίο","","","tCO2Eq","0.52","0.52","0.780","0.780","0.780","0.780","0.780","0.780"]
["","GWP","","","","675","675","675.0","675.0","675.0","675.0","675.0","675.0"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20","20","30","30","30","30","30","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,035 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0035 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15","15","20.0","20.0","20.0","20.0","20.0","20.0"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","","","","","","","","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50","50","50","50"]
["","Τάση","","","V","","","","","","","","220-240"]
["Στάνταρτ εξαρτήματα","Drain cap","","","","","","3","3","3","3","3"]
["Σημειώσεις","","","","","","","","(1) - Δυνατό μόνο σε συνδυασμό με CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","","","","(2) - Δυνατό μόνο σε συνδυασμό με CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9,FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB·","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","","","","","","","","734"]
["","","","Πλάτος","mm","","","","","","","","954"]
["","","","Βάθος","mm","","","","","","","","401"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","","","","","","","","1"]
["","Ετικέτα πλήρωσης ψυκτικού","","","","","","","","","","","1"]
["","Πολύγλωσσες ετικέτες των φθοριούχων αερίων του θερμοκηπίου","","","","","","","","","","","1"]
["","Πώμα εξόδου συμπυκνωμάτων","","","","","","","","","","","3"]
["","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","","","","","","","","","","","1"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","","","","","","","","A+++ ~ D"]
["Σημειώσεις","","","","","","","","","","","","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]