{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","","49.0"]
["","Ψύξη","","Ονομ.","dBA","","49.0"]
["Στάνταρτ εξαρτήματα","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","","","","","1"]
["","Εγχειρίδιο εγκατάστασης","","","","","1"]
["","Ετικέτα πλήρωσης ψυκτικού","","","","","1"]
["","Πολύγλωσσες ετικέτες των φθοριούχων αερίων του θερμοκηπίου","","","","","1"]
["","Γενικές Προφυλάξεις Ασφαλείας","","","","","1"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Φορτίο","","","kg","","0.76"]
["","Τύπος","","","","","R-32"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Μέγ.","°CDB","","50 (4), 46 (5)"]
["","","","Ελάχ.","°CDB","","-10"]
["Piping connections","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","15"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["Συμπιεστής","Type","","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","840"]
["","","","Βάθος","mm","","350"]
["","","","Ύψος","mm","","552"]
["Βάρος","Μονάδα","","","kg","","32"]
["Power supply","Φάση","","","","","1~"]
["","Συχνότητα","","","Hz","","50"]
["","Τάση","","","V","","220-240"]
["Σημειώσεις","","","","","(1) - Δυνατό μόνο σε συνδυασμό με ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["","","","","","(2) - Δυνατό μόνο σε συνδυασμό με ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","","","(4) - Δυνατό μόνο σε συνδυασμό με ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Δυνατό μόνο σε συνδυασμό με ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","552"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","840"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","350"]
["Βάρος","Μονάδα","","","kg","32"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10"]
["","","","Μέγ.","°CDB","50 (4), 46 (5)"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","46.0"]
["","Θέρμανση","","Ονομ.","dBA","47.0"]
["Ψυκτικό μέσο","Φορτίο","","","kg","0.76"]
["","Φορτίο","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Τροφοδοσία ισχύος","Συχνότητα","","","Hz","50"]