{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXP-K3"]
[]
[]
[]
[]
["","","","","","ARXP20K3V1B","ARXP25K3V1B","ARXP35K3V1B"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","550","550","550"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","765","765","765"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","285","285","285"]
["Βάρος","Μονάδα","","","kg","32","32","32"]
["Συμπιεστής","Type","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","46","46","48"]
["","Θέρμανση","","Υψ.","dBA","47","47","48"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32"]
["","Φορτίο","","","kg","0.76","0.76","0.76"]
["","Φορτίο","","","tCO2Eq","0.52","0.52","0.52"]
["","GWP","","","","675","675","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20.0","20.0","20.0"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15.0","15.0","15.0"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240"]