{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","","","47","48"]
["","","","Ονομ.","dBA","","52","","","49"]
["","Ψύξη","","Υψ.","dBA","","","46","48"]
["","","","Ονομ.","dBA","","52","","","49"]
["Στάνταρτ εξαρτήματα","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","","","","","1","1","1","1"]
["","Εγχειρίδιο εγκατάστασης","","","","","1","1","1","1"]
["","Ετικέτα πλήρωσης ψυκτικού","","","","","1","1","","1"]
["","Πολύγλωσσες ετικέτες των φθοριούχων αερίων του θερμοκηπίου","","","","","1","1","","1"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Φορτίο","","","kg","","1.70","1.0","1.2","1.50"]
["","Τύπος","","","","","R-410A","R-410A","R-410A","R-410A"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","σ.α.λ.","","","780","780"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","σ.α.λ.","","","740","740"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Μέγ.","°CDB","","46","46","46","46"]
["","","","Ελάχ.","°CDB","","-10","10","10","-10"]
["","Θέρμανση","Περιβάλλον","Μέγ.","°CWB","","18","18","18","18"]
["","","","Ελάχ.","°CWB","","-15","-15","-15","-15"]
["Piping connections","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","20.0","15","15","20.0"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","65","","","62"]
["","Θέρμανση","","","dBA","","65","","","62"]
["Συμπιεστής","Type","","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","825","765","765","825"]
["","","","Βάθος","mm","","300","285","285","300"]
["","","","Ύψος","mm","","735","550","550","735"]
["Βάρος","Μονάδα","","","kg","","47","34","34","47"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Εξαιρετικά χαμηλές","cfm","","","904","904"]
["","","","Εξαιρετικά χαμηλές","m³/min","","","25.6","25.6"]
["","","Ψύξη","Εξαιρετικά χαμηλές","m³/min","","","30.1","30.1"]
["","","","Εξαιρετικά χαμηλές","cfm","","","1,063","1,063"]
["Power supply","Phase","","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","","50","50","50","50"]
["","Τάση","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Σημειώσεις","","","","","(1) - 220V","","(1) - Κατά τη σύνδεση με σύστημα εξωτερικής μονάδας multi, ανατρέξτε στις προδιαγραφές του συστήματος multi που πρόκειται να συνδεθεί.","(1) - Κατά τη σύνδεση με σύστημα εξωτερικής μονάδας multi, ανατρέξτε στις προδιαγραφές του συστήματος multi που πρόκειται να συνδεθεί."]
["","","","","","(2) - 230V","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","","(3) - 230V","(3) - 230V"]
["","","","","","","","(4) - 240V","(4) - 240V"]
["","","","","","","","(5) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(5) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Εξαιρετικά χαμηλές","m³/min","48.9"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","m³/min","43.1"]
["","","","Εξαιρετικά χαμηλές","cfm","1727"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","cfm","1522"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","735"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","825"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","300"]
["Βάρος","Μονάδα","","","kg","47"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Ψύξη-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","σ.α.λ.","670"]
["","","Θέρμανση","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Θέρμανση-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","σ.α.λ.","670"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","10"]
["","","","Μέγ.","°CDB","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15"]
["","","","Μέγ.","°CWB","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","48"]
["","Θέρμανση","","Υψ.","dBA","48"]
["Ψυκτικό μέσο","Τύπος","","","","R-410A"]
["","Φορτίο","","","kg","1.7"]
["","Φορτίο","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","20"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","220-240"]
["Σημειώσεις","","","","","","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","","","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]