{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","40","42","44","45"]
["","","","Μέτρια","dBA","34","38","40","41"]
["","","","Αθόρυβη λειτουργία","dBA","21","30","32","33"]
["","","","Χαμηλή","dBA","28","33","35","36"]
["","Ψύξη","","Μέτρια","dBA","33","39","41","42"]
["","","","Αθόρυβη λειτουργία","dBA","20","31","33","34"]
["","","","Χαμηλή","dBA","26","34","36","37"]
["","","","Υψ.","dBA","40","43","45","46"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1","1","1"]
["","Εγχειρίδιο χειρισμού","","","","1","1","1","1"]
["","Τηλεχειριστήριο υπερύθρων","","","","1","1","1","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","","2","2","2","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","1","1","1","1"]
["","Πλάκα στήριξης","","","","1","1","1","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","2","2","2","2"]
["Χειριστήρια","Wired remote control","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","9.50","12.7","12.7","12.7"]
["","Drain","","","","18","18","18","18"]
["Απορροφ. ισχύς","Ψύξη","","Ονομ.","kW","0.019","0.029","0.032","0.032"]
["","Θέρμανση","","Ονομ.","kW","0.020","0.032","0.035","0.035"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","55","59","60","62"]
["","Θέρμανση","","","dBA","55","61","62","62"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","770","990","990","990"]
["","","","Βάθος","mm","225","263","263","263"]
["","","","Ύψος","mm","286","295","295","295"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό","Λευκό"]
["Βάρος","Μονάδα","","","kg","8.50","13.5","13.5","13.5"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","10.3","17.3","17.9","17.9"]
["","","","Χαμηλή","m³/min","6.7","12.2","12.8","12.8"]
["","","","Μέτρια","m³/min","8.6","14.8","15.8","15.8"]
["","","","Αθόρυβη λειτουργία","m³/min","5.3","10.7","11.3","11.3"]
["","","Ψύξη","Χαμηλή","m³/min","6.1","11.9","12.2","12.2"]
["","","","Μέτρια","m³/min","8.1","14.4","14.8","14.8"]
["","","","Υψ.","m³/min","10.1","16.8","17.3","17.3"]
["","","","Αθόρυβη λειτουργία","m³/min","4.4","10.5","10.7","10.7"]
["Power supply","Φάση","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50"]
["","Όνομα","","","","","V1","V1","V1"]
["","Τάση","","","V","220-240","220-240","220-240","220-240"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","","","","0.019","0.032"]
["","Θέρμανση","","Ονομ.","kW","","","","","0.02","0.032"]
["Περίβλημα","Χρώμα","","","","","","","","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","","","","","286","286"]
["","","","Πλάτος","mm","","","","","770","770"]
["","","","Βάθος","mm","","","","","225","225"]
["Βάρος","Μονάδα","","","kg","","","","","8.5","9"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","","","","10.1","11.5"]
["","","","Μέτρια","m³/min","","","","","8.1","8.3"]
["","","","Χαμηλή","m³/min","","","","","6.1","6.3"]
["","","","Αθόρυβη λειτουργία","m³/min","","","","","4.4","4.5"]
["","","Θέρμανση","Υψ.","m³/min","","","","","10.3","11.5"]
["","","","Μέτρια","m³/min","","","","","8.6","9"]
["","","","Χαμηλή","m³/min","","","","","6.7","7"]
["","","","Αθόρυβη λειτουργία","m³/min","","","","","5.3","5.3"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","","","","55","58"]
["","Θέρμανση","","","dBA","","","","","55","58"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","","","","40","43"]
["","","","Μέτρια","dBA","","","","","33","34"]
["","","","Χαμηλή","dBA","","","","","26","27"]
["","","","Αθόρυβη λειτουργία","dBA","","","","","20","20"]
["","Θέρμανση","","Υψ.","dBA","","","","","40","40"]
["","","","Μέτρια","dBA","","","","","34","35"]
["","","","Χαμηλή","dBA","","","","","28","29"]
["","","","Αθόρυβη λειτουργία","dBA","","","","","21","21"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","","","","","6.35","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","","","","","9.5","9.5"]
["","Αποχέτευση","","","","","","","","18","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","","","","ARC470A1","ARC470A1"]
["","Τηλεχειριστήριο με καλώδιο","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","","","","","1~","1~"]
["","Συχνότητα","","","Hz","","","","","50","50"]
["","Τάση","","","V","","","","","220-240","220-240"]