{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF42C5V1B","ATXF35C5V1B (Archived)"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","39.0","40.0","44.0"]
["","","","Μέτρια","dBA","34.0","34.0","34.0"]
["","","","Αθόρυβη λειτουργία","dBA","21.0","21.0","22.0"]
["","","","Χαμηλή","dBA","28.0","28.0","28.0"]
["","Ψύξη","","Μέτρια","dBA","33.0","33.0","36.0"]
["","","","Αθόρυβη λειτουργία","dBA","20.0","20.0","22.0"]
["","","","Χαμηλή","dBA","25.0","26.0","30.0"]
["","","","Υψ.","dBA","39.0","40.0","45.0"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1","1"]
["","Εγχειρίδιο χειρισμού","","","","1","1","1"]
["","Μπαταρίες","","","","1","1","1"]
["","Τηλεχειριστήριο υπερύθρων","","","","1","1","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","","2","2","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","1","1","1"]
["","Πλάκα στήριξης","","","","1","1","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","2","2","2"]
["Χειριστήρια","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","χιλ.","6.35","6.35","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","χιλ.","9.50","9.50","9.50"]
["","Αποχέτευση","","","","18","18","18"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.023","0.023","0.040"]
["","Θέρμανση","","Ονομ.","kW","0.023","0.023","0.040"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","53.0","54.0","59.0"]
["","Θέρμανση","","","dBA","55.0","55.0","59.0"]
["Διαστάσεις","Μονάδα","","Πλάτος","χιλ.","770","770","770"]
["","","","Βάθος","χιλ.","225","225","225"]
["","","","Ύψος","χιλ.","286","286","286"]
["Περίβλημα","Colour","","","","Λευκό","Λευκό","Λευκό"]
["Βάρος","Μονάδα","","","kg","8.00","8.00","9.00"]
["Power supply","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","220-440","220-440","220-440"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","","","0.029"]
["","Θέρμανση","","Ονομ.","kW","","","","0.029"]
["Περίβλημα","Χρώμα","","","","","","","Λευκό"]
["Διαστάσεις","Μονάδα","","Ύψος","χιλ.","","","","286"]
["","","","Πλάτος","χιλ.","","","","770"]
["","","","Βάθος","χιλ.","","","","225"]
["Βάρος","Μονάδα","","","kg","","","","8.5"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","","","11.8"]
["","","","Μέτρια","m³/min","","","","8"]
["","","","Χαμηλή","m³/min","","","","6.4"]
["","","","Αθόρυβη λειτουργία","m³/min","","","","4.4"]
["","","Θέρμανση","Υψ.","m³/min","","","","11.9"]
["","","","Μέτρια","m³/min","","","","8.6"]
["","","","Χαμηλή","m³/min","","","","6.5"]
["","","","Αθόρυβη λειτουργία","m³/min","","","","5.3"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","","","54"]
["","Θέρμανση","","","dBA","","","","56"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","","","43"]
["","","","Μέτρια","dBA","","","","34"]
["","","","Χαμηλή","dBA","","","","27"]
["","","","Αθόρυβη λειτουργία","dBA","","","","20"]
["","Θέρμανση","","Υψ.","dBA","","","","40"]
["","","","Μέτρια","dBA","","","","35"]
["","","","Χαμηλή","dBA","","","","29"]
["","","","Αθόρυβη λειτουργία","dBA","","","","21"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","χιλ.","","","","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","χιλ.","","","","9.5"]
["","Αποχέτευση","","","","","","","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","","","ARC470A1"]
["","Τηλεχειριστήριο με καλώδιο","","","","","","","BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","Operation manual","","","","","","","1"]
["","Batteries","","","","","","","1"]
["","Indoor unit fixing screws","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Mounting plate","","","","","","","1"]
["","Remote control holder","","","","","","","1"]
["Τροφοδοσία ισχύος","Φάση","","","","","","","1~"]
["","Συχνότητα","","","Hz","","","","50"]
["","Τάση","","","V","","","","220-440"]