{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3"]
[]
[]
[]
[]
["","","","","","ATXP20K3V1B","ATXP25K3V1B","ATXP35K3V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.017","0.019","0.032"]
["","Θέρμανση","","Ονομ.","kW","0.02","0.02","0.032"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","286","286","286"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","770","770","770"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","225","225","225"]
["Βάρος","Μονάδα","","","kg","9","9","9"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","9.8","10.1","11.5"]
["","","","Μέτρια","m³/min","7.9","8.1","8.3"]
["","","","Χαμηλή","m³/min","5.9","6.1","6.3"]
["","","","Αθόρυβη λειτουργία","m³/min","4.4","4.4","4.5"]
["","","Θέρμανση","Υψ.","m³/min","10.3","10.3","11.5"]
["","","","Μέτρια","m³/min","8.4","8.6","9"]
["","","","Χαμηλή","m³/min","6.5","6.7","7"]
["","","","Αθόρυβη λειτουργία","m³/min","5.3","5.3","5.3"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","55","55","58"]
["","Θέρμανση","","","dBA","55","55","58"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","39","40","43"]
["","","","Μέτρια","dBA","33","33","34"]
["","","","Χαμηλή","dBA","25","26","27"]
["","","","Αθόρυβη λειτουργία","dBA","20","20","20"]
["","Θέρμανση","","Υψ.","dBA","39","40","40"]
["","","","Μέτρια","dBA","34","34","35"]
["","","","Χαμηλή","dBA","28","28","29"]
["","","","Αθόρυβη λειτουργία","dBA","21","21","21"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","6.35","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","9.5","9.5","9.5"]
["","Αποχέτευση","","","","18","18","18"]
["Συστήματα ελέγχου","Infrared remote control","","","","ARC480A11","ARC480A11"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","","ARC480A11"]