{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXTP-K"]
[]
[]
[]
[]
["","","","","","ATXTP25K3V1B","ATXTP35K3V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.03","0.03"]
["","Θέρμανση","","Ονομ.","kW","0.035","0.035"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","285","285"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","770","770"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","225","225"]
["Βάρος","Μονάδα","","","kg","9","9"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","10.6","11.4"]
["","","","Μέτρια","m³/min","7.7","8.2"]
["","","","Χαμηλή","m³/min","5.3","5.4"]
["","","","Αθόρυβη λειτουργία","m³/min","4.3","4.3"]
["","","Θέρμανση","Υψ.","m³/min","11.2","10.8"]
["","","","Μέτρια","m³/min","8","7.8"]
["","","","Χαμηλή","m³/min","5.8","5.8"]
["","","","Αθόρυβη λειτουργία","m³/min","4.9","4.9"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","58","58"]
["","Θέρμανση","","","dBA","58","58"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","43","43"]
["","","","Μέτρια","dBA","35","35"]
["","","","Χαμηλή","dBA","26","26"]
["","","","Αθόρυβη λειτουργία","dBA","21","21"]
["","Θέρμανση","","Υψ.","dBA","43","43"]
["","","","Μέτρια","dBA","35","35"]
["","","","Χαμηλή","dBA","26","26"]
["","","","Αθόρυβη λειτουργία","dBA","21","21"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5","9.5"]
["","Αποχέτευση","","","","16 (εσωτερική διάμετρος εύκαμπτου σωλήνα σύνδεσης)","16 (εσωτερική διάμετρος εύκαμπτου σωλήνα σύνδεσης)"]
["Χειριστήρια","Infrared remote control","","","","ARC480A11","ARC480A11"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1","V1"]
["","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]