{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":9,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MV1"]
[]
[]
[]
[]
["","","","","","AZAS71M2V1B","AZAS100M7V1B","AZAS125M7V1B","AZAS140M7V1B"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","770","990","990","990"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","900","940","940","940"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","320","320","320","320"]
["Βάρος","Μονάδα","","","kg","60","70","70","78"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-5","-5","-5","-5"]
["","","","Μέγ.","°CDB","46","46","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15","-15","-15","-15"]
["","","","Μέγ.","°CWB","15.5","15.5","15.5","15.5"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","65","70","71","73"]
["","Θέρμανση","","","dBA","","","71 (1)","73 (1)"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","46","53","53","54"]
["","Θέρμανση","","Ονομ.","dBA","47","57","57","57"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32","R-32"]
["","Φορτίο","","","kg","2.45","2.60","2.60","2.90"]
["","GWP","","","","675","675","675","675"]
["","Φορτίο","","","tCO2Eq","1.65","1.76","1.76","1.96"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","9.52","9.52","9.52","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","15.9","15.9","15.9","15.9"]
["","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","30","30","30","30"]
["","","Σύστημα","Ισοδύναμο","m","50","50","50","50"]
["","","","Χωρίς φορτίο","m","30","30","30","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","Βλ. εγχειρίδιο εγκατάστασης","Βλ. εγχειρίδιο εγκατάστασης","Βλ. εγχειρίδιο εγκατάστασης","Βλ. εγχειρίδιο εγκατάστασης"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","30.0","30.0","30.0","30.0"]
["","","ΕΣ.-ΕΣ.","Μέγ.","m","0.5","0.5","0.5","0.5"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240"]
["Ρεύμα - 50Hz","Μέγιστα αμπέρ ασφάλειας (MFA)","","","A","20","25","32","32"]
["Στάνταρτ εξαρτήματα","Peel off F-gas label","","","","1"]
["Σημειώσεις","","","","","","","(1) - Σύμφωνα με ENER Lot 21","(1) - Σύμφωνα με ENER Lot 21"]