{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDK"]
[]
[]
[]
[]
["","","","","BRC1HHDAK (Archived)","BRC1HHDAKA (Archived)"]
["Περίβλημα","Χρώμα","","","Μαύρο","Μαύρο"]
["","Κάλυμμα κουμπιών","","","Όχι","Όχι"]
["","LED Λειτουργίας","Χρώμα","","Μπλε ενδεικτική λυχνία","Μπλε ενδεικτική λυχνία"]
["Διαστάσεις","Μονάδα","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","85","85"]
["","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","85","85"]
["","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","25","25"]
["","Μονάδα με στεγανοποίηση","Διαστάσεις-=-Μονάδα με στεγανοποίηση-=-Ύψος-=-χιλ.","mm","50","50"]
["","","Διαστάσεις-=-Μονάδα με στεγανοποίηση-=-Πλάτος-=-χιλ.","mm","217","217"]
["","","Διαστάσεις-=-Μονάδα με στεγανοποίηση-=-Βάθος-=-χιλ.","mm","161","161"]
["Βάρος","Μονάδα","","kg","0.110","0.110"]
["","Μονάδα με στεγανοποίηση","","kg","0.317","0.317"]
["Συσκευασία","Υλικό","","","Χαρτόνι","Χαρτόνι"]
["","Βάρος","","kg","0.0850","0.0850"]
["LCD","Τύπος","","","100 x 150 εικονοστοιχεία","100 x 150 εικονοστοιχεία"]
["","Διαστάσεις","Ύψος","mm","40.7","40.7"]
["","","Πλάτος","mm","28.0","28.0"]
["","Οπίσθια λυχνία","Χρώμα","","Λευκό","Λευκό"]
["Θερμοκρασία περιβάλλοντος","Λειτουργία","Ελάχ.","°C","-10","-10"]
["","","Μέγ.","°C","50","50"]
["","Φύλαξη","Ελάχ.","°C","-20","-20"]
["","","Μέγ.","°C","70","70"]
["","Θερμοκρασία περιβάλλοντος-=-Σχετική υγρασία <-=-%","","%","95","95"]
["Συστήματα ελέγχου","Κατηγορία ελέγχου θερμοκρασίας","","","VI","VI"]
["","Συνεισφορά στην εποχιακή απόδοση θέρμανσης χώρου","","%","4.0","4.0"]
["Συνδέσεις καλωδιώσεων","Μήκος καλωδίου","Μέγ.","m","500","500"]