{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CKHWS-BV3"]
[]
[]
[]
[]
["","","","","","CKHWS180BJV3","CKHWS230BJV3"]
["Διαστάσεις","Μονάδα","Ύψος","Δεξαμενή","mm","1655","1855"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","595","595"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","634","634"]
["Βάρος","Μονάδα","","Κενό","kg","106","115"]
["Δεξαμενή","Όγκος νερού","","","l","180","230"]
["","Υλικό","","","","Ανοξείδωτος χάλυβας (ΕΝ 1.4521)","Ανοξείδωτος χάλυβας (ΕΝ 1.4521)"]
["","Μέγιστη θερμοκρασία νερού","","","°C","65.0","65.0"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","","B","B"]
["Εφεδρικός θερμαντήρας","Απόδοση","","","kW","1.5","1.5"]
["Σημειώσεις","","","","","(1) - Με βάση το dT 45 K","(1) - Με βάση το dT 45 K"]
["","","","","","(2) - Ροή DHW","(2) - Ροή DHW"]
["","","","","","(3) - 2-πολική 10A, καμπύλη 230V","(3) - 2-πολική 10A, καμπύλη 230V"]
["","","","","","(4) - Η παραπάνω τροφοδοσία ρεύματος του κιβωτίου hydro είναι μόνο για τον εφεδρικό θερμαντήρα. Το κιβώτιο διακοπτών και η αντλία του υδρο-κιβωτίου παρέχονται μέσω της εξωτερικής μονάδας.","(4) - Η παραπάνω τροφοδοσία ρεύματος του κιβωτίου hydro είναι μόνο για τον εφεδρικό θερμαντήρα. Το κιβώτιο διακοπτών και η αντλία του υδρο-κιβωτίου παρέχονται μέσω της εξωτερικής μονάδας."]