{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Στάθμη ηχ. πίεσης","Θέρμανση","Υψ.","dBA","39"]
["","","Μέτρια","dBA","32"]
["","","Αθόρυβη λειτουργία","dBA","21"]
["","","Χαμηλή","dBA","25"]
["","Ψύξη","Medium","dBA","32"]
["","","Αθόρυβη λειτουργία","dBA","21"]
["","","Χαμηλή","dBA","25"]
["","","Υψ.","dBA","39"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","1"]
["","Εγχειρίδιο χειρισμού","","","1"]
["","Φίλτρο αέρα","","","2"]
["","Τηλεχειριστήριο υπερύθρων","","","1"]
["","Πλάκα στήριξης τηλεχειριστηρίου","","","1"]
["","Βιδωτή σακούλα","","","1"]
["","Βιδωτό κάλυμμα","","","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","2"]
["","Γενικές Προφυλάξεις Ασφαλείας","","","1"]
["Ψυκτικό μέσο","GWP","","","675.0"]
["Συστήματα ελέγχου","Τηλεχειριστήριο με καλώδιο","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35"]
["","Αερίου","Εξ.Διάμ.","mm","9.50"]
["","Drain","","","18"]
["Ισχύς εισόδου","Ψύξη","Ονομ.","kW","0.020"]
["","Θέρμανση","Ονομ.","kW","0.020"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","57"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","798"]
["","","Βάθος","mm","189"]
["","","Ύψος","mm","295"]
["Περίβλημα","Χρώμα","","","Blackwood"]
["Βάρος","Μονάδα","","kg","12"]
["Power supply","Φάση","","","1~"]
["","Συχνότητα","","Hz","50"]
["","Όνομα","","","V1"]
["","Τάση","","V","220-240"]