{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CB"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BB"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.020"]
["","Θέρμανση","","Ονομ.","kW","0.020"]
["Περίβλημα","Χρώμα","","","","Μαύρο"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","295"]
["","","","Πλάτος","mm","798"]
["","","","Βάθος","mm","189"]
["Βάρος","Μονάδα","","","kg","11.5"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","11.0"]
["","","","Μέτρια","m³/min","8.2"]
["","","","Χαμηλή","m³/min","6.1"]
["","","","Αθόρυβη λειτουργία","m³/min","4.6"]
["","","Θέρμανση","Υψ.","m³/min","10.9"]
["","","","Μέτρια","m³/min","8.7"]
["","","","Χαμηλή","m³/min","6.4"]
["","","","Αθόρυβη λειτουργία","m³/min","4.5"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","57"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","39"]
["","","","Μέτρια","dBA","32"]
["","","","Χαμηλή","dBA","25"]
["","","","Αθόρυβη λειτουργία","dBA","21"]
["","Θέρμανση","","Υψ.","dBA","39"]
["","","","Μέτρια","dBA","32"]
["","","","Χαμηλή","dBA","25"]
["","","","Αθόρυβη λειτουργία","dBA","21"]
["Ψυκτικό μέσο","GWP","","","","675.0"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","9.50"]
["","Συμπυκνωμάτων","","","","18"]
["Χειριστήρια","Infrared remote control","","","","ARC466A85"]
["","Τηλεχειριστήριο με καλώδιο","","","","BRC073A1"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1"]
["","Εγχειρίδιο χειρισμού","","","","1"]
["","Φίλτρο αέρα","","","","2"]
["","Τηλεχειριστήριο υπερύθρων","","","","1"]
["","Πλάκα στήριξης τηλεχειριστηρίου","","","","1"]
["","Βιδωτή σακούλα","","","","1"]
["","Βιδωτό κάλυμμα","","","","2"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","","2"]
["","Γενικές Προφυλάξεις Ασφαλείας","","","","1"]
["Power supply","Όνομα","","","","V1"]
["","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","220-240"]