{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.029","0.029"]
["","Θέρμανση","","Ονομ.","kW","0.023","0.023"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","295","295"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","778","778"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","272","272"]
["Βάρος","Μονάδα","","","kg","10","10"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","10.5","10.5"]
["","","","Μέτρια","m³/min","7.5","7.5"]
["","","","Χαμηλή","m³/min","5.7","5.7"]
["","","","Αθόρυβη λειτουργία","m³/min","4.3","4.3"]
["","","Θέρμανση","Υψ.","m³/min","9.3","9.3"]
["","","","Μέτρια","m³/min","8.2","8.2"]
["","","","Χαμηλή","m³/min","6.2","6.2"]
["","","","Αθόρυβη λειτουργία","m³/min","5.1","5.1"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","57","57"]
["","Θέρμανση","","","dBA","54","54"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","41","41"]
["","","","Μέτρια","dBA","33","33"]
["","","","Χαμηλή","dBA","25","25"]
["","","","Αθόρυβη λειτουργία","dBA","19","19"]
["","Θέρμανση","","Υψ.","dBA","39","39"]
["","","","Μέτρια","dBA","34","34"]
["","","","Χαμηλή","dBA","26","26"]
["","","","Αθόρυβη λειτουργία","dBA","20","20"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5","9.5"]
["","Αποχέτευση","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC466A67","ARC466A67"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC073A1","BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1","V1"]
["","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]