{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Θερμοκρασία περιβάλλοντος","Σχετική υγρασία <","","","%","85"]
["Μέγιστος αριθμός εσωτερικών μονάδων που μπορούν να συνδεθούν","","","","","32"]
["Ισχύς εισόδου","kW","","","","0.015 (1)"]
["Επικοινωνία","DIII-NET","","Ποσότητα","","1"]
["","","","Παρατήρηση","","DIII-NET (F1F2)"]
["","Ethernet","","Ποσότητα","","1"]
["","Ακροδέκτης εισόδου","Ψηφιακό","Ποσότητα","","4"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","384"]
["","","","Βάθος","mm","92"]
["","","","Ύψος","mm","136"]
["Μέγιστος αριθμός εξωτερικών μονάδων που μπορούν να συνδεθούν","","","","","7"]
["Power supply","Συχνότητα","","","Hz","50/60"]
["","Τάση","","","V","110-240 AC"]
["Σημειώσεις","","","","","(1) - Περιλαμβάνει την ισχύ εισόδου της παροχής ισχύος WAGO, της μονάδας CPU και της μονάδας Ι/Ο"]
["","","","","","(2) - Οι διαστάσεις περιλαμβάνουν την παροχή ισχύος WAGO, τις μονάδες CPU, τη μονάδα Ι/Ο και τον απαιτούμενο χώρο μεταξύ των διαφορετικών τμημάτων"]
["","","","","","(3) - Η διάσταση της προαιρετικής οθόνης είναι: ύψος: 209 mm, πλάτος: 123 mm, βάθος: 8,5 mm"]