{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSH-D"]
[]
[]
[]
[]
["","","","","","EBSH11P30DF","EBSH11P50DF","EBSH11P30DG","EBSH11P50DG","EBSH16P30DF","EBSH16P50DF","EBSH16P30DG","EBSH16P50DG"]
["Περίβλημα","Χρώμα","","","","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)"]
["","Υλικό","","","","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","1,893","1,910","1,893","1,910","1,893","1,910","1,893","1,910"]
["","","","Πλάτος","mm","594","792","594","792","594","792","594","792"]
["","","","Βάθος","mm","680","817","680","817","680","817","680","817"]
["Βάρος","Μονάδα","","","kg","93","114","93","114","93","114","93","114"]
["PED","Κατηγορία","","","","Κατηγορία II","Κατηγορία II","Κατηγορία II","Κατηγορία II","Κατηγορία II","Κατηγορία II","Κατηγορία II","Κατηγορία II"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Φορτίο","","","kg","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Φορτίο","","","tCO2Eq","2.57","2.57","2.57","2.57","2.57","2.57","2.57","2.57"]
["Στάθμη ηχητικής ισχύος","Ονομ.","","","dBA","44.7","44.7","44.7","44.7","49.0","49.0","49.0","49.0"]
["Στάθμη ηχητικής πίεσης","Ονομ.","","","dBA","36.8","36.8","36.8","36.8","40.3","40.3","40.3","40.3"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Ελάχ.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Μέγ.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Πλευρά νερού","Ελάχ.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Μέγ.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50","50","50","50"]
["","Τάση","","","V","230","230","230","230","230","230","230","230"]
["Σημειώσεις","","","","","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897"]
["","","","","","(2) - Ανατρέξτε στα όρια λειτουργίας στο σχέδιο","(2) - Ανατρέξτε στα όρια λειτουργίας στο σχέδιο","(2) - Ανατρέξτε στα όρια λειτουργίας στο σχέδιο","(2) - Ανατρέξτε στα όρια λειτουργίας στο σχέδιο","(2) - Ανατρέξτε στα όρια λειτουργίας στο σχέδιο","(2) - Ανατρέξτε στα όρια λειτουργίας στο σχέδιο","(2) - Ανατρέξτε στα όρια λειτουργίας στο σχέδιο","(2) - Ανατρέξτε στα όρια λειτουργίας στο σχέδιο"]