{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBVZ-D6V"]
[]
[]
[]
[]
["","","","","","EBVZ16S18DJ6V","EBVZ16S23DJ6V"]
["Περίβλημα","Χρώμα","","","","Λευκή + Μαύρη","Λευκή + Μαύρη"]
["","Υλικό","","","","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","1655","1855"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","595","595"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","634","634"]
["Βάρος","Μονάδα","","","kg","137","145"]
["PED","Κατηγορία","","","","Κατηγορία II","Κατηγορία II"]
["Στάθμη ηχητικής ισχύος","Ονομ.","","","dBA","44.0","44.0"]
["Στάθμη ηχητικής πίεσης","Ονομ.","","","dBA","30.0","30.0"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Ελάχ.","°C","15","15"]
["","","","Μέγ.","°C","60","60"]
["","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","10","10"]
["","","Πλευρά νερού","Ελάχ.","°C","5","5"]
["","","","Μέγ.","°C","22","22"]
["Τροφοδοσία ισχύος","Όνομα","","","","Βλ. σημείωση 6","Βλ. σημείωση 6"]
["Ηλεκτρικός θερμαντήρας","Τροφοδοσία ισχύος","","Όνομα","","6V3","6V3"]
["","","","Φάση","","1~ / 3~","1~ / 3~"]
["","","","Συχνότητα","Hz","50","50"]
["","","","Τάση","V","230","230"]
["","Συνιστώμενες ασφάλειες","","","A","20","20"]
["Σημειώσεις","","","","","(1) - Ο τομέας λειτουργίας επεκτείνεται στις χαμηλότερες ταχύτητες ροής ανάλογα με την κατάσταση λειτουργίας - ανατρέξτε στην καμπύλη ESP.","(1) - Ο τομέας λειτουργίας επεκτείνεται στις χαμηλότερες ταχύτητες ροής ανάλογα με την κατάσταση λειτουργίας - ανατρέξτε στην καμπύλη ESP."]
["","","","","","(2) - Με βάση dT 45 K","(2) - Με βάση dT 45 K"]
["","","","","","(3) - συμπεριλαμβανομένων σωληνώσεων + PHE + εφεδρικός θερμαντήρας / εξαιρείται το δοχείο διαστολής","(3) - συμπεριλαμβανομένων σωληνώσεων + PHE + εφεδρικός θερμαντήρας / εξαιρείται το δοχείο διαστολής"]
["","","","","","(4) - Μέτρηση με μια πτώση πίεσης 10 kPa στο σύστημα θέρμανσης σε συνθήκες λειτουργίας νερού εξόδου 47-55°C σε χώρο με θερμοκρασία περιβάλλοντος 20°C. DB/WB 7°C/6°.","(4) - Μέτρηση με μια πτώση πίεσης 10 kPa στο σύστημα θέρμανσης σε συνθήκες λειτουργίας νερού εξόδου 47-55°C σε χώρο με θερμοκρασία περιβάλλοντος 20°C. DB/WB 7°C/6°."]
["","","","","","(5) - Για περισσότερες λεπτομέρειες, δείτε το σχέδιο εύρους λειτουργίας","(5) - Για περισσότερες λεπτομέρειες, δείτε το σχέδιο εύρους λειτουργίας"]
["","","","","","(6) - 4 πόλοι 20 Α καμπύλη 400V κατηγορία ενεργοποίησης C (ανατρέξτε στο διάγραμμα συνδεσμολογίας)","(6) - 4 πόλοι 20 Α καμπύλη 400V κατηγορία ενεργοποίησης C (ανατρέξτε στο διάγραμμα συνδεσμολογίας)"]