{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EDLA-D3W17"]
[]
[]
[]
[]
["","","","","","EDLA16DA3W17"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","16.0 (1) (2)"]
["Απόδοση θερμαντήρα","Βήμα 1","","","kW","3"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","3.53 (1), 4.56 (2)"]
["COP","","","","","4.53 (1), 3.51 (2)"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","870"]
["","","","Πλάτος","mm","1380"]
["","","","Βάθος","mm","460"]
["Βάρος","Μονάδα","","","kg","149"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","85.0"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Ελάχ.","°C","15 (6)"]
["","","","Μέγ.","°C","60 (6)"]
["","Ζεστό νερό χρήσης","Περιβάλλοντος","Ελάχ.","°CDB","-25"]
["","","","Μέγ.","°CDB","35"]
["","","Πλευρά νερού","Ελάχ.","°C","25"]
["","","","Μέγ.","°C","55 (6)"]
["Ψυκτικό μέσο","Τύπος","","","","R-32"]
["","GWP","","","","675"]
["","Φορτίο","","","kg","3.80"]
["","Φορτίο","","","tCO2Eq","2.57"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","SCOP","","3.33"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A++"]
["","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","SCOP","","4.62"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A+++"]
["Εξάρτημα συμπιεστή","Γενική τροφοδοσία ρεύματος","","Φάση","","3N~"]
["","","","Τάση","V","400"]
["Τροφοδοσία ισχύος","Όνομα","","","","W1"]
["","Φάση","","","","3~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","400"]
["Σημειώσεις","","","","","(1) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Ψύξη: EW 12°C; LW 7°C; συνθήκες περιβάλλοντος: 35°CDB"]
["","","","","","(4) - Ψύξη: EW 23°C; LW 18°C; συνθήκες περιβάλλοντος: 35°CDB"]
["","","","","","(5) - Κατά EN14825"]
["","","","","","(6) - Για περισσότερες λεπτομέρειες, δείτε το σχέδιο εύρους λειτουργίας"]
["","","","","","(7) - Εξαρτάται από την κατάσταση λειτουργίας,  συμβουλευθείτε το εγχειρίδιο εγκατάστασης."]