{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EDLA09-14D3W1"]
[]
[]
[]
[]
["","","","","","EDLA09DA3W1","EDLA11DA3W1","EDLA14DA3W1"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","9.37 (1), 9.00 (2)","10.6 (1), 9.82 (2)","12.0 (1), 12.5 (2)"]
["Απόδοση θερμαντήρα","Βήμα 1","","","kW","3","3","3"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","1.91 (1), 2.43 (2)","2.18 (1), 2.68 (2)","2.46 (1), 3.42 (2)"]
["COP","","","","","4.91 (1), 3.71 (2)","4.83 (1), 3.66 (2)","4.87 (1), 3.64 (2)"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","870","870","870"]
["","","","Πλάτος","mm","1380","1380","1380"]
["","","","Βάθος","mm","460","460","460"]
["Βάρος","Μονάδα","","","kg","149","149","149"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","48.0","55.8","70.4"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Ελάχ.","°C","15 (6)","15 (6)","15 (6)"]
["","","","Μέγ.","°C","60 (6)","60 (6)","60 (6)"]
["","Ζεστό νερό χρήσης","Περιβάλλοντος","Ελάχ.","°CDB","-25","-25","-25"]
["","","","Μέγ.","°CDB","35","35","35"]
["","","Πλευρά νερού","Ελάχ.","°C","25","25","25"]
["","","","Μέγ.","°C","55 (6)","55 (6)","55 (6)"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32"]
["","GWP","","","","675","675","675"]
["","Φορτίο","","","kg","3.80","3.80","3.80"]
["","Φορτίο","","","tCO2Eq","2.57","2.57","2.57"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","SCOP","","3.39","3.32","3.37"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A++","A++","A++"]
["","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","SCOP","","4.72","4.64","4.62"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A+++","A+++","A+++"]
["Εξάρτημα συμπιεστή","Γενική τροφοδοσία ρεύματος","","Φάση","","3N","3N~","3N~"]
["","","","Τάση","V","400","400","400"]
["Τροφοδοσία ισχύος","Όνομα","","","","W1","W1","W1"]
["","Φάση","","","","3~","3~","3~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","400","400","400"]
["Σημειώσεις","","","","","(1) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Για περισσότερες λεπτομέρειες, δείτε το σχέδιο εύρους λειτουργίας","(3) - Για περισσότερες λεπτομέρειες, δείτε το σχέδιο εύρους λειτουργίας","(3) - Για περισσότερες λεπτομέρειες, δείτε το σχέδιο εύρους λειτουργίας"]
["","","","","","(4) - Εξαρτάται από την κατάσταση λειτουργίας,  συμβουλευθείτε το εγχειρίδιο εγκατάστασης.","(4) - Εξαρτάται από την κατάσταση λειτουργίας,  συμβουλευθείτε το εγχειρίδιο εγκατάστασης.","(4) - Εξαρτάται από την κατάσταση λειτουργίας,  συμβουλευθείτε το εγχειρίδιο εγκατάστασης."]