{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-E"]
[]
[]
[]
[]
["","","","","","EHSH04P30EF","EHSH04P30EG","EHSH08P30EF","EHSH08P50EF","EHSH08P30EG","EHSH08P50EG"]
["Περίβλημα","Χρώμα","","","","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)"]
["","Υλικό","","","","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","1,892","1,891","1,892","1,905","1,891","1,910"]
["","","","Πλάτος","mm","594","594","594","792","594","792"]
["","","","Βάθος","mm","644","644","644","812","644","817"]
["Βάρος","Μονάδα","","","kg","77","77.0","77","107","77.0","97.0"]
["PED","Κατηγορία","","","","Είδος 4.3","Είδος 4.3","Είδος 4.3","Είδος 4.3","Είδος 4.3","Είδος 4.3"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675","675.0","675","675","675.0","675.0"]
["","Φορτίο","","","kg","1.5","1.50","1.5","1.5","1.50","1.50"]
["Στάθμη ηχητικής ισχύος","Ονομ.","","","dBA","39","39","39","39","39","39"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Ελάχ.","°C","18","18","18","18","18","18"]
["","","","Μέγ.","°C","65","65","65","65","65","65"]
["","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","10","10","10","10","10","10"]
["","","Πλευρά νερού","Ελάχ.","°C","5","5","5","5","5","5"]
["","","","Μέγ.","°C","22","22","22","22","22","22"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50","50"]
["","Τάση","","","V","230","230","230","230","230","230"]
["Σημειώσεις","","","","","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897"]