{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","EHYHBH05AFV32","EHYHBH05AAV32","EHYHBH08AFV32","EHYHBH08AAV32"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό","Λευκό"]
["","Υλικό","","","","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","902","902","902","902"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","450","450","450","450"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","164","164","164","164"]
["Βάρος","Μονάδα","","","kg","30.0","30.0","31.2","31.2"]
["PED","Κατηγορία","","","","ΑΕ. 3§3, Εξαιρείται από το πλαίσιο της PED (Οδηγία για συσκευές πίεσης) λόγω του άρθρου 1, στοιχείο 3.6 της 97/23/EC","ΑΕ. 3§3, Εξαιρείται από το πλαίσιο της PED (Οδηγία για συσκευές πίεσης) λόγω του άρθρου 1, στοιχείο 3.6 της 97/23/EC","Κατηγορία Ι","Κατηγορία Ι"]
["Εναλλάκτης θερμότητας πλευράς νερού","Ταχύτητα ροής νερού","Θέρμανση","Μέγ.","l/min","23.0 (7)","23.0","23.5 (7)","23.5"]
["Στάθμη ηχητικής ισχύος","Ονομ.","","","dBA","42.0","42.0","42.0","42.0"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Ελάχ.","°C","25 (8)","25","25 (8)","25"]
["","","","Μέγ.","°C","55 (8)","55","55 (8)","55"]
["Τροφοδοσία ισχύος","Όνομα","","","","V3","V3","V3","V3"]
["","Φάση","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50"]
["","Τάση","","","V","230","230","230","230"]
["Συνδέσεις καλωδιώσεων","Για σύνδεση με διασύνδεση χρήστη","","Ποσότητα","","2","2","2","2"]
["","","","Παρατήρηση","","0,75 mm² έως 1,25 mm² (μέγ. μήκος 500m)","0,75 mm² έως 1,25 mm² (μέγ. μήκος 500m)","0,75 mm² έως 1,25 mm² (μέγ. μήκος 500m)","0,75 mm² έως 1,25 mm² (μέγ. μήκος 500m)"]
["Σημειώσεις","","","","","(1) - Μόνο για εσωτερική μονάδα","","(1) - Μόνο για εσωτερική μονάδα"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), παράκαμψη μπόιλερ","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), παράκαμψη μπόιλερ"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), παράκαμψη μπόιλερ","","(3) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), παράκαμψη μπόιλερ"]
["","","","","","(4) - Min. required","","(4) - Min. required"]
["","","","","","(5) - Παράκαμψη μπόιλερ","","(5) - Παράκαμψη μπόιλερ"]
["","","","","","(6) - Για το εύρος λειτουργίας των *HYHB* και *HYKOMB33AA, δείτε το σχέδιο εύρους λειτουργίας","","(6) - Για το εύρος λειτουργίας των *HYHB* και *HYKOMB33AA, δείτε το σχέδιο εύρους λειτουργίας"]