{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AFV3"]
["Περίβλημα","Χρώμα","","","","Λευκό"]
["","Υλικό","","","","Λαμαρίνα με επικάλυψη"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","902"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","450"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","164"]
["Βάρος","Μονάδα","","","kg","31.2"]
["PED","Κατηγορία","","","","Κατηγορία Ι"]
["Εναλλάκτης θερμότητας πλευράς νερού","Ταχύτητα ροής νερού","Θέρμανση","Μέγ.","l/min","23.5 (7)"]
["Στάθμη ηχητικής ισχύος","Ονομ.","","","dBA","42.0"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Ελάχ.","°C","25 (8)"]
["","","","Μέγ.","°C","55 (8)"]
["","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","10 (8)"]
["","","Πλευρά νερού","Ελάχ.","°C","5 (8)"]
["","","","Μέγ.","°C","22 (8)"]
["Τροφοδοσία ισχύος","Όνομα","","","","V3"]
["","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","230"]
["Συνδέσεις καλωδιώσεων","Για σύνδεση με διασύνδεση χρήστη","","Ποσότητα","","2"]
["","","","Παρατήρηση","","0,75 mm² έως 1,25 mm² (μέγ. μήκος 500m)"]
["Σημειώσεις","","","","","(1) - Μόνο για εσωτερική μονάδα"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), παράκαμψη μπόιλερ"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), παράκαμψη μπόιλερ"]
["","","","","","(4) - Tamb 35°C - LWE 7°C (DT=5°C), παράκαμψη μπόιλερ"]
["","","","","","(5) - Tamb 35°C - LWE 18°C (DT=5°C), παράκαμψη μπόιλερ"]
["","","","","","(6) - Min. required"]
["","","","","","(7) - Παράκαμψη μπόιλερ"]
["","","","","","(8) - Για το εύρος λειτουργίας των *HYHB* και *HYKOMB33AA, δείτε το σχέδιο εύρους λειτουργίας"]