{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":71,"n_cols":7,"rows_kept":71,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHE-CV3"]
[]
[]
[]
[]
["","","","","","EKHHE200CV3","EKHHE260CV3"]
["Sound power level","Θέρμανση ζεστού νερού χρήσης","","Εσωτερική μονάδα","dBA","50","50"]
["","","","Εξωτερική μονάδα","dBA","49","49"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A+","A+"]
["","","","Ρύθμιση θερμοκρασίας θερμοστάτη","°C","55","55"]
["","","","Λειτουργία για την ρύθμιση της θέρμανσης νερού κατά τη διάρκεια των ωρών εκτός αιχμής","","Ναι","Ναι"]
["","","","Δηλωμένο προφίλ φορτίου","","L","XL"]
["","Ψυχρό κλίμα","","AEC (ετήσια κατανάλωση ηλεκτρικού ρεύματος)","kWh","979","1,672"]
["","","","Qelec (ημερήσια κατανάλωση ηλεκτρικού ρεύματος)","kWh","2.68","4.58"]
["","Θερμό κλίμα","","Qelec (ημερήσια κατανάλωση ηλεκτρικού ρεύματος)","kWh","1.91","3.10"]
["","","","AEC (ετήσια κατανάλωση ηλεκτρικού ρεύματος)","kWh","698","1,132"]
["","Μέσο κλίμα","","Qelec (ημερήσια κατανάλωση ηλεκτρικού ρεύματος)","kWh","2.08","3.30"]
["","","","AEC (ετήσια κατανάλωση ηλεκτρικού ρεύματος)","kWh","758","1,203"]
["Αντλία θερμότητας","Εύρος λειτουργίας","Περιβάλλον","Ελάχ.","°CDB","-7","-7"]
["","","","Μέγ.","°CDB","43","43"]
["","Casing","","Χρώμα","","Λευκό","Λευκό"]
["","Πίεση συστήματος","","Μέγ.","bar","7","7"]
["","Μέθοδος απόψυξης","","","","Απόψυξη θερμού αερίου","Απόψυξη θερμού αερίου"]
["","Απόδοση θέρμανσης","","","kW","0.43","0.43"]
["","Εγκατάσταση","","Απόσταση από τον τοίχο","χιλ.","200","200"]
["","","","Κατηγορία ΙΡ","","IP24","IP24"]
["","Βάρος","","Μονάδα","kg","85","97"]
["","","","Μονάδα με στεγανοποίηση","kg","96","109"]
["","Τοποθεσία εγκατάστασης","","","","Εσωτερική μονάδα μόνο","Εσωτερική μονάδα μόνο"]
["","Στάθμη ηχητικής πίεσης","","Νυχτερινή αθόρυβη λειτουργία","dBA","50.0","50.0"]
["","","","Ονομ.","dBA","50","50"]
["","Όνομα","","","","EKHHE200CV3","EKHHE260CV3"]
["","Ψυκτικό μέσο","","GWP","","1,430","1,430"]
["","","","Φορτίο","kg","1","1"]
["","","","Τύπος","","R-134A","R-134A"]
["","Διαστάσεις","Μονάδα","Βάθος","χιλ.","628","628"]
["","","","Πλάτος","χιλ.","628","628"]
["","","","Ύψος","χιλ.","1,607","1,892"]
["COP","","","","","4.23","4.23"]
["Ψυκτικό μέσο","GWP","","","","1,430","1,430"]
["","Φορτίο","","","kg","1","1"]
["","Τύπος","","","","R-134a","R-134a"]
["Compressor","Type","","","","Περιστροφικός","Περιστροφικός"]
["Διαστάσεις","Μονάδα","","Διάμετρος","χιλ.","628","628"]
["","","","Ύψος","χιλ.","1,607","1,892"]
["","","Ύψος","Ενσωματωμένη στην εσωτερική μονάδα","χιλ.","1,607","1,892"]
["Ζεστό νερό χρήσης","Έξοδος","","Ονομ.","kW","1.82","1.82"]
["Δεξαμενή","Εγκατάσταση","","Δυνατότητα σύνδεσης θερμικού ηλιακού συστήματος","","Όχι","Όχι"]
["","","","Κατηγορία ΙΡ","","IP24","IP24"]
["","","","Άνοιγμα ανακυκλοφορίας δεξαμενής","","όχι","όχι"]
["","Ενσωματωμένη ισχύς θερμαντικού στοιχείου","","Ονομ.","kW","1.5","1.5"]
["","Τοποθεσία εγκατάστασης","","","","Εσωτερική μονάδα μόνο","Εσωτερική μονάδα μόνο"]
["","Περίβλημα","","Υλικό","","Επισμαλτωμένος χάλυβας","Επισμαλτωμένος χάλυβας"]
["","","","Χρώμα","","Λευκό","Λευκό"]
["Βάρος","Μονάδα με στεγανοποίηση","","","kg","96","109"]
["","Μονάδα","","Κενό","kg","85","97"]
["Τοποθεσία εγκατάστασης","","","","","Εσωτερική","Εσωτερική"]
["General","LW(A) Στάθμη ηχητικής ισχύoς (σύμφωνη με το EN14825)","","Εσωτερικός χώρος","dB(A)","50","50"]
["","Product description","","Αντλία θερμότητας αέρα σε νερό","","Ναι","Ναι"]
["","","","Model identifier","","EKHHE200CV3","EKHHE260CV3"]
["","Λεπτομέρειες προμηθευτή/κατασκευαστή","","Ονομασία ή εμπορικό σήμα","","Daikin Europe N.V.","Daikin Europe N.V."]
["","Συμπληρωματικός θερμαντήρας","","Τύπος ενέργειας εισόδου","","Ηλεκτρικό","Ηλεκτρικό"]
["Χρόνος θέρμανσης","Μέγ.","","","ωω:λλ","08:17:00","10:14:00"]
["Αντλία θερμότητας","Τροφοδοσία ισχύος","","Συχνότητα","Hz","50","50"]
["","","","Μέγιστο ρεύμα λειτουργίας","A","8.5","8.5"]
["","","","Φάση","","1P","1P"]
["","","","Τάση","V","230","230"]
["","","","Προτεινόμενη χρήση εγκατάστασης","A","2.43","2.43"]
["Δεξαμενή","Τροφοδοσία ισχύος","","Φάση","","1P","1P"]
["","","","Συχνότητα","Hz","50","50"]
["","","","Τάση","V","230","230"]