{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSV-P"]
[]
[]
[]
[]
["","","","","EKSV21P","EKSV21P1","EKSV26P","EKSV26P1"]
["Διάταξη απορρόφησης","","","","Ένδειξη σωλήνα χαλκού σε σχήμα άρπας με επενδυμένη αλουμινένια πλάκα υψηλής επιλογής με συγκόλληση λέιζερ","Ένδειξη σωλήνα χαλκού σε σχήμα άρπας με επενδυμένη αλουμινένια πλάκα υψηλής επιλογής με συγκόλληση λέιζερ","Ένδειξη σωλήνα χαλκού σε σχήμα άρπας με επενδυμένη αλουμινένια πλάκα υψηλής επιλογής με συγκόλληση λέιζερ","Ένδειξη σωλήνα χαλκού σε σχήμα άρπας με επενδυμένη αλουμινένια πλάκα υψηλής επιλογής με συγκόλληση λέιζερ"]
["Θερμοκρασία ακινητοποίησης","Μέγ.","","°C","192","192","192","192"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","85","1,006","85","1,300"]
["","","Βάθος","mm","2,000","85","2,000","85"]
["","","Ύψος","mm","1,006","2,000","1,300","2,000"]
["Πίεση λειτουργίας","Μέγ.","","bar","6","6","6","6"]
["Βάρος","Μονάδα","","kg","33","35","42","42"]
["Επιφανείας","Άνοιγμα","","m²","1.800","1.800","2.360","2.360"]
["","Απορροφητής","","m²","1.79","1.80","2.35","2.36"]
["","Εξωτερικό","","m²","2.01","2.01","2.60","2.60"]
["Στερέωση","","","","Κατακόρυφος","Κατακόρυφος","Κατακόρυφος","Κατακόρυφος"]
["Υαλοπίνακας","","","","Γυαλί ασφαλείας μονού υαλοπίνακα, μετάδοση +/- 92%","Γυαλί ασφαλείας μονού υαλοπίνακα, μετάδοση +/- 92%","Γυαλί ασφαλείας μονού υαλοπίνακα, μετάδοση +/- 92%","Γυαλί ασφαλείας μονού υαλοπίνακα, μετάδοση +/- 92%"]
["Επιτρεπόμενη γωνία οροφής","Μέγ.","","°","80","80","80","80"]
["","Ελάχ.","","°","15","15","15","15"]
["Επικάλυψη","","","","Micro-therm (Μικροθερμικό) (απορρόφηση μέγ. 96%, εκπομπές περ. 5% +/-2%)","Micro-therm (Μικροθερμικό) (απορρόφηση μέγ. 96%, εκπομπές περ. 5% +/-2%)","Micro-therm (Μικροθερμικό) (απορρόφηση μέγ. 96%, εκπομπές περ. 5% +/-2%)","Micro-therm (Μικροθερμικό) (απορρόφηση μέγ. 96%, εκπομπές περ. 5% +/-2%)"]
["Όγκος","l","","","1.3","1.3","1.7","1.7"]
["Θερμική απόδοση","Απόδοση συλλέκτη με μηδενική απώλεια η0","","%","0.781","0.710","0.784","0.710"]
["","Συντελεστής απώλειας θερμότητας a1","","W/m².K","4.240","4.300","4.250","4.300"]
["","Συνάρτηση θερμοκρασίας του συντελεστή απώλειας θερμότητας a2","","W/m².K²","0.006","0.006","0.007","0.006"]
["","Θερμική ικανότητα","","kJ/K","4.9","4.9","6.5","6.5"]