{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERSQ-AV1"]
[]
[]
[]
[]
["","","","","","ERSQ011AAV1","ERSQ014AAV1","ERSQ016AAV1"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","","53"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","","1"]
["Ψυκτικό μέσο","GWP","","","","","2,087.5"]
["","Charge","","","kg","","4.5"]
["","Τύπος","","","","","R-410A"]
["Εύρος λειτουργίας","Heating","","Max.","°CWB","","20"]
["","","","Min.","°CWB","","-20"]
["","Ζεστό νερό χρήσης","","Ελάχ.","°CDB","","-20"]
["","","","Μέγ.","°CDB","","35"]
["Συνδέσεις σωληνώσεων","Θερμομόνωση","","","","","Σωληνώσεις υγρού και σωληνώσεις αερίου"]
["","Υγρό","","ΕΞ.ΔΙΑΜ.","χιλ.","","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","χιλ.","","15.9"]
["","Συμπυκνωμάτων","","Εξ.Διάμ.","χιλ.","","26x3"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","30"]
["Στάθμη ηχητικής ισχύος","Heating","","Ονομ.","dBA","","69"]
["Διαστάσεις","Μονάδα","","Πλάτος","χιλ.","","900"]
["","","","Βάθος","χιλ.","","320"]
["","","","Ύψος","χιλ.","","1,345"]
["Βάρος","Μονάδα","","","kg","","120"]
["Power supply","Φάση","","","","","1~"]
["","Όνομα","","","","","V1"]
["","Συχνότητα","","","Hz","","50"]
["","Τάση","","","V","","220-440"]
["Ρεύμα","Συνιστώμενες ασφάλειες","","","A","","25"]
["Σημειώσεις","","","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","","(2) - Zmax: Σύμφωνα με το EN/IEC 61000-3-11, ενδέχεται να είναι απαραίτητο να συμβουλευθείτε το διαχειριστή δικτύου διανομής προκειμένου να διασφαλίσετε ότι ο εξοπλισμός είναι συνδεδεμένος μόνο σε δίκτυο τροφοδοσίας με Zsys (σύνθετη αντίσταση συστήματος) μικρότερη ή ίση με Zmax"]
["","","","","","","(3) - EN/IEC 61000-3-11: Ευρωπαϊκό/Διεθνές τεχνικό πρότυπο για τα όρια των μεταβολών τάσης,  διακυμάνσεων τάσεις και αναβόσβημα που παράγονται από δημόσιο σύστημα χαμηλής τάσης με ρεύμα εισόδου ≤ 75A"]
["","","","","","","(4) - Ελάχιστη τιμή Ssc (=Ισχύς βραχυκυκλώματος): Εξοπλισμός σύμμορφος με το πρότυπο EN/IEC 61000-3-12: Ευρωπαϊκό/ διεθνές τεχνικό πρότυπο για τον καθορισμό των ορίων αρμονικών ρευμάτων που παράγει εξοπλισμός συνδεδεμένος σε δημόσια δίκτυα χαμηλής τάσης με ρεύμα εισόδου  > 16A και ≤ 75A ανά φάση"]
["","","","","","","(5) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","1345","","1345"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","900","","900"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","320","","320"]
["Βάρος","Μονάδα","","","kg","120","","120"]
["Εύρος λειτουργίας","Θέρμανση","","Ελάχ.","°CWB","-20","","-20"]
["","","","Μέγ.","°CWB","20","","20"]
["","Ζεστό νερό χρήσης","","Ελάχ.","°CDB","-20","","-20"]
["Εύρος λειτ.","Ζεστό νερό χρ.","","Μέγ.","°CDB","35","","35"]
["Στάθμη ηχητικής ισχύος","Θέρμανση","","Ονομ.","dBA","68","","71"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","52","","55"]
["Ψυκτικό μέσο","Τύπος","","","","R-410A","","R-410A"]
["","GWP","","","","2087.5","","2087.5"]
["","Φορτίο","","","tCO2Eq","9.4","","9.4"]
["","Φορτίο","","","kg","4.5","","4.5"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","9.52","","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","15.9","","15.9"]
["","Συμπυκνωμάτων","","Εξ.Διάμ.","χιλ.","26x3","","26x3"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","30","","30"]
["","Θερμομόνωση","","","","Σωληνώσεις υγρού και σωληνώσεις αερίου","","Σωληνώσεις υγρού και σωληνώσεις αερίου"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1","","V1"]
["","Φάση","","","","1~","","1~"]
["","Συχνότητα","","","Hz","50","","50"]
["","Τάση","","","V","220-440","","220-440"]
["Ρεύμα","Συνιστώμενες ασφάλειες","","","A","25","","25"]