{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERSQ-AY1"]
[]
[]
[]
[]
["","","","","","ERSQ011AAY1","ERSQ014AAY1","ERSQ016AAY1"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","52","53","55"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1","1"]
["Ψυκτικό μέσο","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Φορτίο","","","kg","4.5","4.5","4.5"]
["","Τύπος","","","","R-410A","R-410A","R-410A"]
["Εύρος λειτουργίας","Θέρμανση","","Μέγ.","°CWB","20","20","20"]
["","","","Ελάχ.","°CWB","-20","-20","-20"]
["","Ζεστό νερό χρήσης","","Ελάχ.","°CDB","-20","-20","-20"]
["","","","Μέγ.","°CDB","35","35","35"]
["Συνδέσεις σωληνώσεων","Θερμομόνωση","","","","Σωληνώσεις υγρού και σωληνώσεις αερίου","Σωληνώσεις υγρού και σωληνώσεις αερίου","Σωληνώσεις υγρού και σωληνώσεις αερίου"]
["","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","15.9","15.9","15.9"]
["","Συμπυκνωμάτων","","Εξ.Διάμ.","mm","26x3","26x3","26x3"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","30","30","30"]
["Sound power level","Heating","","Ονομ.","dBA","68","69","71"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","900","900","900"]
["","","","Βάθος","mm","320","320","320"]
["","","","Ύψος","mm","1,345","1,345","1,345"]
["Βάρος","Μονάδα","","","kg","120","120","120"]
["Power supply","Φάση","","","","3~","3~","3~"]
["","Όνομα","","","","Y1","Y1","Y1"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","380-415","380-415","380-415"]
["Ρεύμα","Συνιστώμενες ασφάλειες","","","A","16","16","16"]
["Σημειώσεις","","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","(2) - Ssc: Ισχύς βραχυκυκλώσεως","(2) - Ssc: Ισχύς βραχυκυκλώσεως","(2) - Ssc: Ισχύς βραχυκυκλώσεως"]
["","","","","","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]