{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":12,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWAD-TZXRC2"]
[]
[]
[]
[]
["","","","","","EWADC15TZXRC2","EWADH17TZXRC2","EWADH16TZXRC2","EWADC11TZXRC2","EWADH12TZXRC2","EWADC12TZXRC2","EWADC14TZXRC2"]
["Απόδοση ψύξης","Ονομ.","","","kW","1,499","1,735","1,625","1,122","1,279","1,204","1,362"]
["Έλεγχος απόδοσης","Μέθοδος","","","","Μεταβλητή","Μεταβλητή","Μεταβλητή","Μεταβλητή","Μεταβλητή","Μεταβλητή","Μεταβλητή"]
["","Ελάχιστη απόδοση","","","%","12.5","12.5","12.5","12.5","12.5","12.5","12.5"]
["Power input","Ψύξη","","Ονομ.","kW","501.4","598.6","547.6","356.3","403","377.3","450.1"]
["EER","","","","","2.99","2.90","2.97","3.15","3.17","3.19","3.03"]
["IPLV","","","","","5.65","5.6","5.64","5.51","5.49","5.55","5.64"]
["SEER","","","","","5.31","5.32","5.31","5.30","5.32","5.33","5.27"]
["Διαστάσεις","Μονάδα","","Βάθος","mm","12,302","14,104","13,202","10,510","12,302","11,402","11,402"]
["","","","Ύψος","mm","2,540","2,540","2,540","2,540","2,540","2,540","2,540"]
["","","","Πλάτος","mm","2,282","2,282","2,282","2,282","2,282","2,282","2,282"]
["Βάρος","Βάρος λειτουργίας","","","kg","12,145","13,048","12,575","9,879","11,526","11,123","11,727"]
["","Μονάδα","","","kg","11,134","12,037","11,564","9,322","10,515","10,112","10,716"]
["Περίβλημα","Colour","","","","Κρεμ_","Κρεμ_","Κρεμ_","Κρεμ_","Κρεμ_","Κρεμ_","Κρεμ_"]
["","Υλικό","","","","Γαλβανισμένο και βαμμένο χαλυβδοέλασμα","Γαλβανισμένο και βαμμένο χαλυβδοέλασμα","Γαλβανισμένο και βαμμένο χαλυβδοέλασμα","Γαλβανισμένο και βαμμένο χαλυβδοέλασμα","Γαλβανισμένο και βαμμένο χαλυβδοέλασμα","Γαλβανισμένο και βαμμένο χαλυβδοέλασμα","Γαλβανισμένο και βαμμένο χαλυβδοέλασμα"]
["Εναλλάκτης θερμότητας αέρα","Τύπος","","","","Μικροκανάλι","Μικροκανάλι","Μικροκανάλι","Μικροκανάλι","Μικροκανάλι","Μικροκανάλι","Μικροκανάλι"]
["Ανεμιστήρας","Ποσότητα","","","","26","30","28","22","26","24","24"]
["","Type","","","","Απευθείας έλικα","Απευθείας έλικα","Απευθείας έλικα","Απευθείας έλικα","Απευθείας έλικα","Απευθείας έλικα","Απευθείας έλικα"]
["Κιν. ανεμιστήρα","Μετάδοση κίνησης","","","","Οδηγείται με VFD","Οδηγείται με VFD","Οδηγείται με VFD","Οδηγείται με VFD","Οδηγείται με VFD","Οδηγείται με VFD","Οδηγείται με VFD"]
["Compressor","Ποσότητα_","","","","2","2","2","2","2","2","2"]
["","Type","","","","Συμπιεστής κοχλιωτού τύπου (single screw) Inverter","Συμπιεστής κοχλιωτού τύπου (single screw) Inverter","Συμπιεστής κοχλιωτού τύπου (single screw) Inverter","Συμπιεστής κοχλιωτού τύπου (single screw) Inverter","Συμπιεστής κοχλιωτού τύπου (single screw) Inverter","Συμπιεστής κοχλιωτού τύπου (single screw) Inverter","Συμπιεστής κοχλιωτού τύπου (single screw) Inverter"]
["","Starting method","","","","Οδηγείται με VFD","Οδηγείται με VFD","Οδηγείται με VFD","Οδηγείται με VFD","Οδηγείται με VFD","Οδηγείται με VFD","Οδηγείται με VFD"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","Ονομ.","dBA","94","95","95","92","94","93","93"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","71","72","71","70","71","70","71"]
["Ψυκτικό μέσο","Τύπος","","","","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a"]
["","GWP","","","","1,430","1,430","1,430","1,430","1,430","1,430","1,430"]
["","Φορτίο","","","kg","220","270","250","175","220","200","200"]
["","Κυκλώματα","","Ποσότητα","","2","2","2","2","2","2","2"]
["Piping connections","Είσοδος/έξοδος νερού εξατμιστή (Εξ. Διάμ.)","","","","273","273","273","219.1","219.1","273","273"]
["Power supply","Phase","","","","3~","3~","3~","3~","3~","3~","3~"]
["","Συχνότητα","","","Hz","50","50","50","50","50","50","50"]
["","Τάση","","","V","400","400","400","400","400","400","400"]
["","Εύρος τάσης","","Ελάχ.","%","-1","-1","-1","-1","-1","-1","-1"]
["","","","Μέγ.","%","-1","-1","-1","-1","-1","-1","-1"]
["Μονάδα","Ρεύμα εκκίν.","","Μέγ.","A","0.0","0.0","0.0","0.0","0.0","0.0","0.0"]
["","Ρεύμα λειτ.","Ψύξη","Ονομ.","A","834.0","982.6","901.3","612.3","689.6","651.0","762.5"]
["","","","Μέγ.","A","1,124","1,313","1,218","918","994","939","1,085"]
["","Μέγ. ένταση ρεύματος μονάδας για μέγεθος των καλωδίων","","","A","1,236","1,444","1,340","1,010","1,093","1,033","1,194"]