{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWLS-J-SS"]
[]
[]
[]
[]
["","","","","EWLS110J-SS","EWLS130J-SS","EWLS150J-SS","EWLS170J-SS","EWLS200J-SS","EWLS240J-SS","EWLS270J-SS"]
["Απόδοση ψύξης","Ονομ.","","kW","111","132","150","175","200","236","268"]
["Έλεγχος απόδοσης","Μέθοδος","","","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless","Stepless"]
["","Ελάχιστη απόδοση","","%","25","25","25","25","25","25","25"]
["Ισχύς εισόδου","Ψύξη","Ονομ.","kW","32.2","38.7","44.8","51.2","58.2","69.4","78.8"]
["EER","","","","3.44","3.41","3.35","3.41","3.44","3.41","3.4"]
["Διαστάσεις","Μονάδα","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","2684","2684","2684","2684","2684","2684","2684"]
["","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","1020","1020","1020","1020","1020","1020","1020"]
["","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","913","913","913","913","913","913","913"]
["Βάρος","Μονάδα","","kg","1124","1141","1237","1263","1305","1489","1489"]
["","Βάρος λειτουργίας","","kg","1138","1159","1253","1281","1327","1518","1518"]
["Εναλλάκτης θερμότητας νερού - εξατμιστής","Τύπος","","","Εναλλάκτης θερμότητας πλάκας","Εναλλάκτης θερμότητας πλάκας","Εναλλάκτης θερμότητας πλάκας","Εναλλάκτης θερμότητας πλάκας","Εναλλάκτης θερμότητας πλάκας","Εναλλάκτης θερμότητας πλάκας","Εναλλάκτης θερμότητας πλάκας"]
["","Όγκος νερού","","l","14","18","14","17","20","26","26"]
["Συμπιεστής","Τύπος","","","Κοχλιοφόρος (single screw) συμπιεστής","Κοχλιοφόρος (single screw) συμπιεστής","Κοχλιοφόρος (single screw) συμπιεστής","Κοχλιοφόρος (single screw) συμπιεστής","Κοχλιοφόρος (single screw) συμπιεστής","Κοχλιοφόρος (single screw) συμπιεστής","Κοχλιοφόρος (single screw) συμπιεστής"]
["Συμπιεστής","Ποσότητα","","","1","1","1","1","1","1","1"]
["Στάθμη ηχητικής ισχύος","Ψύξη","Ονομ.","dBA","88.9","88.9","88.9","88.9","88.9","88.9","88.9"]
["Στάθμη ηχητικής πίεσης","Ψύξη","Ονομ.","dBA","79","79","79","79","79","79","79"]
["Ψυκτικό μέσο","Τύπος","","","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A"]
["","Κυκλώματα","Ψυκτικό μέσο-=-Κυκλώματα-=-Ποσότητα","","1","1","1","1","1","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","3~","3~","3~","3~","3~","3~","3~"]
["","Συχνότητα","","Hz","50","50","50","50","50","50","50"]
["","Τάση","","V","400","400","400","400","400","400","400"]