{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBQ71C8VEB / RZQSG71L3V1B","FBQ100C8VEB / RZQSG100L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG100L9V1B","FBQ50C8VEB / FBQ50C8VEB / RZQSG100L9V1B","FBQ125C8VEB / RZQSG125L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG125L9V1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQSG125L9V1B","FBQ60C8VEB / FBQ60C8VEB / RZQSG125L9V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","6.8","9.5","","","12.0"]
["Ψύξη χώρου","SEER","","","5.81","5.50","5.10","5.10","5.20","4.80","4.80","4.80"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","410","605","652","652","808","875","875","875"]
["","Απόδοση","Pdesign","kW","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A+","A","B","B","A","B","B","B"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","6.00","7.60","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.88","4.01","3.80","3.80","3.90","3.80","3.80","3.80"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A","A+","A","A","A","A","A","A"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","2,166","2,654","2,800","2,800","2,729","2,800","2,800","2,800"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","1,035","1,435","","","1,870"]
["","EER","","","3.28","3.31","","","3.21"]
["","COP","","","3.61","3.65","","","3.51"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A","","","A"]
["","","Θέρμανση","","A","A","","","B"]
["Απόδοση θέρμανσης","Ονομ.","","kW","7.5","10.8","","","13.5"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]
["","","","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]