{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D"]
[]
[]
[]
[]
["","","","","","FBQ35D2VEB","FBQ50D2VEB","FBQ60D2VEB","FBQ71D2VEB","FBQ100D2VEB","FBQ125D2VEB","FBQ140D2VEB"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","37","37","31","31.0","36.0","38.0","38"]
["","","","Μέτρια","dBA","34","34","28","28.0","33.0","35.0","35"]
["","","","Χαμηλή","dBA","29","29","25","25.0","30.0","32.0","32"]
["","Ψύξη","","Μέτρια","dBA","32","32","28","28.0","32.0","35.0","35"]
["","","","Χαμηλή","dBA","29","29","25","25.0","30.0","32.0","32"]
["","","","Υψ.","dBA","35","35","30","30.0","34.0","37.0","37"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο χειρισμού","","","","1","1","1","1","1","1","1"]
["","Εγχειρίδιο εγκατάστασης","","","","1","1","1","1","1","1","1"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","","1","1","1","1","1","1","1"]
["","Μεταλλικός σφιγκτήρας εύκαμπτου σωλήνα αποστράγγισης συμπυκνωμάτων","","","","1","1","1","1","1","1","1"]
["","Ροδέλα για στήριγμα ανάρτησης","","","","8","8","8","8","8","8","8"]
["","Κοχλίες","","","","40","40","40","40","40","40","40"]
["","Μόνωση συνδέσμου","","","","2","2","2","2","2","2","2"]
["","Στεγανοποιητικό παρέμβυσμα","","","","5","5","5","5","5","5","5"]
["","Φύλλα στεγανοποίησης","","","","","","","5","5","5","5"]
["","Σφιγκτήρες","","","","4","4","4","4","4","4","4"]
["Ψυκτικό μέσο","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","","","","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528"]
["","Infrared remote control","","","","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Συμπυκνωμάτων","","","","VP20 (Εσ. διαμ. 20/Εξ.Διάμ. 26), ύψος αποστράγγισης 625 mm","VP20 (Εσ. διαμ. 20/Εξ.Διάμ. 26), ύψος αποστράγγισης 625 mm","VP20 (Εσ. διαμ. 20/Εξ.Διάμ. 26), ύψος αποστράγγισης 625 mm","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Ψύξη","","","dBA","60","60","56","56","58","62","62"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","700","700","1,000","1,000","1,400","1,400","1,400"]
["","","","Βάθος","mm","800","800","800","800","800","800","800"]
["","","","Ύψος","mm","245","245","245","245","245","245","245"]
["Περίβλημα","Υλικό","","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["","Χρώμα","","","","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)"]
["Βάρος","Μονάδα","","","kg","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Ανεμιστήρας","Εξωτερική στατική πίεση","","Υψηλή","Pa","150","150","150","150","150","150","150"]
["","","","Ονομ.","Pa","30","30","30","30","40","50","50"]
["","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","","","","","29.0","34.0","34.0"]
["","","","Χαμηλή","m³/min","","","","","23.0","23.5","23.5"]
["","","","Μέτρια","m³/min","","","","","26.0","29.0","29.0"]
["","","Ψύξη","Χαμηλή","m³/min","","","","","23.0","23.5","23.5"]
["","","","Μέτρια","m³/min","","","","","26.0","29.0","29.0"]
["","","","Υψ.","m³/min","","","","","29.0","34.0","34.0"]
["Ύψος αντλίας συμπυκνωμάτων","mm","","","","625","625","625","625","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Όνομα","","","","VE","VE","VE","VE","VE","VE","VE"]
["","Τάση","","","V","220-240","220-240","220-240","220-240/220","220-240/220","220-240/220","220-240/220"]
["Σημειώσεις","","","","","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]