{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":13,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Απόδοση ψύξης","Ονομ.","","kW","","","","","","6.80 (1)","","","13.4 (1)"]
["Ψύξη χώρου","SEER","","","","","","","6.91","6.91","","","6.75"]
["","ηs, c","","%","","","","","","","","","266.9"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","","","","345","345","","","1,191"]
["","Απόδοση","Pdesign","kW","","","","","6.80","6.80","","","13.4"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","","","","","A++","A++"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","","","","","7.60","7.60","","","11.8"]
["","SCOP/A","","","","","","","4.54","4.54","","","4.38"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","","","","","A+","A+"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","","","","2,344","2,344","","","3,766"]
["","ηs,h","","%","","","","","","","","","172.1"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","","","","","","830"]
["","EER","","","","","","","","4.09 (3)","","","3.18 (3)"]
["","COP","","","","","","","","4.80 (3)","","","4.12 (3)"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","","","","","","A"]
["","","Θέρμανση","","","","","","","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","","","","","","7.50 (2)","","","15.5 (2)"]
["Εύρος ενεργειακής αποδοτικότητας","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D"]
["Σημειώσεις","","","","","","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 7,5m / υψομετρική διαφορά: 0m","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 7,5m / υψομετρική διαφορά: 0m"]
["","","","","","","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 7,5m / υψομετρική διαφορά: 0m","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 7,5m / υψομετρική διαφορά: 0m"]
["","","","","","","","","","(3) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","","","(3) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["Outdoor unit","","","","","","","","","","RZQG100L8Y1","RZQG125L8Y1"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","","","","","","","A","A"]
["","Απόδοση","Pdesign","kW","","","","","","","9.50","12.0"]
["","SEER","","","","","","","","","5.10","5.10"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","","","","","","652","824"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","","","","","","","A","A"]
["","Απόδοση","Pdesign","kW","","","","","","","11.30","12.71"]
["","SCOP/A","","","","","","","","","3.80","3.80"]
["","Pdh Θερμαντική απόδοση στους -10°","","kW","","","","","","","9.66","11.4"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","","","","","","4164","4683"]