{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":117,"n_cols":9,"rows_kept":117,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F"]
[]
[]
[]
[]
["","","","","","FCQHG71FVEB","FCQHG100FVEB","FCQHG125FVEB","FCQHG140FVEB"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","","44","45","45"]
["","","","Ονομ.","dBA","","39","40","41"]
["","","","Χαμηλή","dBA","","33","35","37"]
["","Ψύξη","","Χαμηλή","dBA","","33","35","37"]
["","","","Υψ.","dBA","","44","45","45"]
["","","","Ονομ.","dBA","","39","40","41"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο χειρισμού","","","","","Εγχειρίδιο χειρισμού","Εγχειρίδιο χειρισμού","Εγχειρίδιο χειρισμού"]
["","Εγχειρίδιο εγκατάστασης","","","","","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","","","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων"]
["","Σφιγκτήρας εύκαμπτου σωλήνα αποστράγγισης συμπυκνωμάτων","","","","","Σφιγκτήρας εύκαμπτου σωλήνα αποστράγγισης συμπυκνωμάτων","Σφιγκτήρας εύκαμπτου σωλήνα αποστράγγισης συμπυκνωμάτων","Σφιγκτήρας εύκαμπτου σωλήνα αποστράγγισης συμπυκνωμάτων"]
["","Ροδέλα για στήριγμα ανάρτησης","","","","","Ροδέλα για στήριγμα ανάρτησης","Ροδέλα για στήριγμα ανάρτησης","Ροδέλα για στήριγμα ανάρτησης"]
["","Κοχλίες","","","","","Κοχλίες","Κοχλίες","Κοχλίες"]
["","Οδηγός εγκατάστασης","","","","","Οδηγός εγκατάστασης","Οδηγός εγκατάστασης","Οδηγός εγκατάστασης"]
["","Μόνωση συνδέσμου","","","","","2","2","2"]
["","Φύλλα στεγανοποίησης","","","","","4","4","4"]
["","Στεγανοποιητικό παρέμβυσμα εξόδου συμπυκν.","","","","","Στεγανοποιητικό παρέμβυσμα εξόδου συμπυκν.","Στεγανοποιητικό παρέμβυσμα εξόδου συμπυκν.","Στεγανοποιητικό παρέμβυσμα εξόδου συμπυκν."]
["","Σφιγκτήρες","","","","","Σφιγκτήρες","Σφιγκτήρες","Σφιγκτήρες"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","","9.52","9.52","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","","15.9","15.9","15.9"]
["","Συμπυκνωμάτων","","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Διακοσμητική μάσκα 4","Διαστάσεις","","Βάθος","mm","","50","50","50"]
["","","","Πλάτος","mm","","950","950","950"]
["","","","Ύψος","mm","","950","950","950"]
["","Μοντέλο","","","","","BYCQ140D7W1 - λευκό με γκρι γρίλιες","BYCQ140D7W1 - λευκό με γκρι γρίλιες","BYCQ140D7W1 - λευκό με γκρι γρίλιες"]
["","Χρώμα","","","","","Κατάλευκο (RAL 9010)","Κατάλευκο (RAL 9010)","Κατάλευκο (RAL 9010)"]
["","Βάρος","","","kg","","5.4","5.4","5.4"]
["Sound power level","Ψύξη","","","dBA","","61","61","61"]
["","Θέρμανση","","","dBA","","61","61","61"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","840","840","840"]
["","","","Βάθος","mm","","840","840","840"]
["","","","Ύψος","mm","","288","288","288"]
["Περίβλημα","Υλικό","","","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["Βάρος","Μονάδα","","","kg","","26","26","26"]
["Διακοσμητική μάσκα","Βάρος","","","kg","","10.3","10.3","10.3"]
["","Μοντέλο","","","","","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα"]
["","Διαστάσεις","","Ύψος","mm","","130","130","130"]
["","","","Βάθος","mm","","950","950","950"]
["","","","Πλάτος","mm","","950","950","950"]
["","Χρώμα","","","","","Λευκό (RAL 9010)","Λευκό (RAL 9010)","Λευκό (RAL 9010)"]
["Power supply","Φάση","","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","","50","50","50"]
["","Όνομα","","","","","VE","VE","VE"]
["","Τάση","","","V","","220-240","220-240","220-240"]
["Σημειώσεις","","","","","","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]
["","","","","","","(2) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται.","(2) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται.","(2) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται."]
["","","","","","","(3) - BYCQ140D7W1: Στάνταρ πάνελ σε κατάλευκο με γκρι γρίλιες. BYCQ140D7W1W: Στάνταρ πάνελ σε κατάλευκο με λευκές γρίλιες. BYCQ140D7GW1: Πάνελ αυτο-καθαρισμού σε κατάλευκο.","(3) - BYCQ140D7W1: Στάνταρ πάνελ σε κατάλευκο με γκρι γρίλιες. BYCQ140D7W1W: Στάνταρ πάνελ σε κατάλευκο με λευκές γρίλιες. BYCQ140D7GW1: Πάνελ αυτο-καθαρισμού σε κατάλευκο.","(3) - BYCQ140D7W1: Στάνταρ πάνελ σε κατάλευκο με γκρι γρίλιες. BYCQ140D7W1W: Στάνταρ πάνελ σε κατάλευκο με λευκές γρίλιες. BYCQ140D7GW1: Πάνελ αυτο-καθαρισμού σε κατάλευκο."]
["Περίβλημα","Υλικό","","","","Γαλβανισμένο χαλυβδοέλασμα"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","288"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","840"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","840"]
["Βάρος","Μονάδα","","","kg","25"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","21.2"]
["","","","Ονομ.","m³/min","16.7"]
["","","","Χαμηλή","m³/min","12.2"]
["","","Θέρμανση","Υψ.","m³/min","21.2"]
["","","","Ονομ.","m³/min","16.7"]
["","","","Χαμηλή","m³/min","12.2"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","53"]
["","Θέρμανση","","","dBA","53"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","36"]
["","","","Ονομ.","dBA","33"]
["","","","Χαμηλή","dBA","29"]
["","Θέρμανση","","Υψ.","dBA","36"]
["","","","Ονομ.","dBA","33"]
["","","","Χαμηλή","dBA","29"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","15.9"]
["","Αποχέτευση","","","","VP25 (I.D. 25/O.D. 32)"]
["Διακοσμητική μάσκα","Μοντέλο","","","","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα"]
["","Χρώμα","","","","Λευκό (RAL 9010)"]
["","Διαστάσεις","","Διακοσμητική μάσκα-=-Διαστάσεις-=-Ύψος-=-χιλ.","mm","130"]
["","","","Διακοσμητική μάσκα-=-Διαστάσεις-=-Πλάτος-=-χιλ.","mm","950"]
["","","","Διακοσμητική μάσκα-=-Διαστάσεις-=-Βάθος-=-χιλ.","mm","950"]
["","Βάρος","","","kg","10.3"]
["Διακοσμητική μάσκα 2","Μοντέλο","","","","BYCQ140D7GW1 - Μάσκα αυτοκαθαρισμού"]
["","Χρώμα","","","","Λευκό (RAL 9010)"]
["","Διαστάσεις","","Διακοσμητική μάσκα 2-=-Διαστάσεις-=-Ύψος-=-χιλ.","mm","130"]
["","","","Πλάτος","mm","950"]
["","","","Βάθος","mm","950"]
["","Βάρος","","","kg","10.3"]
["Διακοσμητική μάσκα 3","Μοντέλο","","","","BYCQ140D7W1W - Εντελώς λευκή"]
["","Χρώμα","","","","Λευκό (RAL 9010)"]
["","Διαστάσεις","","Ύψος","mm","50"]
["","","","Πλάτος","mm","950"]
["","","","Βάθος","mm","950"]
["","Βάρος","","","kg","5.4"]
["Διακοσμητική μάσκα 4","Μοντέλο","","","","BYCQ140D7W1 - Λευκή με γκρίζα πτερύγια"]
["","Χρώμα","","","","Λευκό (RAL 9010)"]
["","Διαστάσεις","","Ύψος","mm","950"]
["","","","Πλάτος","mm","950"]
["","","","Βάθος","mm","50"]
["","Βάρος","","","kg","5.4"]
["Χειριστήρια","Infrared remote control","","","","BRC7FA532F"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC1D52, BRC1E52A/B"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","Installation manual"]
["","Washer for hanger bracket","","","","Washer for hanger bracket"]
["","Operation manual","","","","Operation manual"]
["","Clamp for drain hose","","","","Clamp for drain hose"]
["","Clamps","","","","Clamps"]
["","Drain hose","","","","Drain hose"]
["","Drain sealing pad","","","","Drain sealing pad"]
["","Installation guide","","","","Installation guide"]
["","Insulation for fitting","","","","2"]
["","Screws","","","","Screws"]
["","Sealing pads","","","","4"]
["Τροφοδοσία ισχύος","Όνομα","","","","VE"]
["","Φάση","","","","1~"]
["","Τροφοδοσία ισχύος-=-Συχνότητα","","Συχνότητα","","50"]
["","Τροφοδοσία ισχύος-=-Τάση","","Τάση","","220-240"]