{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F"]
[]
[]
[]
[]
["","","","","","FDXM35F2V1B"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Ονομ.","m³/min","8.0"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","33"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Ονομ.","m³/min","8.0"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","33"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.036"]
["","Θέρμανση","","Ονομ.","kW","0.036"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","200"]
["","","","Πλάτος","mm","750"]
["","","","Βάθος","mm","620"]
["Βάρος","Μονάδα","","","kg","21"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","8.7"]
["","","","Χαμηλή","m³/min","7.3"]
["","","Θέρμανση","Υψ.","m³/min","8.7"]
["","","","Χαμηλή","m³/min","7.3"]
["","Εξωτερική στατική πίεση","","Ονομ.","Pa","30"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","53"]
["","Θέρμανση","","","dBA","53"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","35"]
["","","","Χαμηλή","dBA","27"]
["","Θέρμανση","","Υψ.","dBA","35"]
["","","","Χαμηλή","dBA","27"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","9.5"]
["","Αποχέτευση","","","","VP20 (I.D. 20/O.D. 26)"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","BRC4C65"]
["","Τηλεχειριστήριο με καλώδιο","","","","BRC1D52, BRC1E51A"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1"]
["","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","230"]