{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-N"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXM50N2V1B","FDXM60F3V1B / RXM60N2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","","1.70"]
["","Ονομ.","","kW","","6.00"]
["","Μέγ.","","kW","","6.50"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","","1.70"]
["","Ονομ.","","kW","","7.00"]
["","Μέγ.","","kW","","7.10"]
["Ονομαστική απόδοση","EER","","","","2.93"]
["","COP","","","","3.21"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","","1,024"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","","C"]
["","","Θέρμανση","","","C"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","","A"]
["","Απόδοση","Pdesign","kW","","6.00"]
["","SEER","","","","5.56"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","378"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","","A"]
["","Απόδοση","Pdesign","kW","","4.60"]
["","SCOP/A","","","","3.80"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","1,693"]
["Σημειώσεις","","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","","(3) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσ. θερμοκρ.: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m"]
["","","","","","(4) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.70"]
["","Ονομ.","","kW","5.00"]
["","Μέγ.","","kW","5.30"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","1.70"]
["","Ονομ.","","kW","5.80"]
["","Μέγ.","","kW","6.00"]
["Ονομαστική απόδοση","EER","","","3.06"]
["","COP","","","3.10"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","816"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","B"]
["","","Θέρμανση","","D"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A+"]
["","Απόδοση","Pdesign","kW","5.00"]
["","SEER","","","5.77"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","303"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A"]
["","Απόδοση","Pdesign","kW","4.00"]
["","SCOP/A","","","3.93"]
["","Pdh Θερμαντική απόδοση στους -10°","","kW","3.55"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","1424"]
["Εύρος ενεργειακής αποδοτικότητας","","","","A+++ ~ D"]