{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-C / RXS-F"]
[]
[]
[]
[]
["","","","","FDXS60CVMB / RXS60F3V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.7"]
["","Μέγ.","","kW","6.5"]
["","Ονομ.","","kW","6.0 (1)"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","χιλ.","6.35"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","χιλ.","12.7"]
["","Συμπυκνωμάτων","OD","χιλ.","26"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","1,065"]
["","EER","","","2.82"]
["","COP","","","3.02"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","C"]
["","","Θέρμανση","","D"]
["Απόδοση θέρμανσης","Ονομ.","","kW","7.0 (2)"]
["","Ελάχ.","","kW","1.7"]
["","Μέγ.","","kW","8.0"]
["Σημειώσεις","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, 24°CWB, ισοδύναμο μήκος σωληνώσεων: 7,5m"]
["","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 7,5m"]
["","","","","(3) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]