{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-E / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS25E7VMB / RXS25K2V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","2.40 (3)"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","9.5"]
["","Drain","OD","mm","VP20 (Εξωτερική διάμ. 26, Εσωτερική διάμ. 20)"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","345"]
["","EER","","","3.48"]
["","COP","","","3.52"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A"]
["","","Θέρμανση","","B"]
["Απόδοση θέρμανσης","Ονομ.","","kW","3.20 (4)"]
["Σημειώσεις","","","","(1) - Ενεργειακή σήμανση: κλίμακα από A (περισσότερο αποδοτικό) έως G (λιγότερο αποδοτικό)"]
["","","","","(2) - Ετήσια κατανάλωση ενέργειας: βασισμένη σε μέση ετήσια χρήση 500 ωρών λειτουργίας υπό πλήρες φορτίο (ονομαστικές συνθήκες)"]
["","","","","(3) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19,0°CWB / εξ. θερμοκρασία 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m / υψομετρική διαφορά: 0m"]
["","","","","(4) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m / υψομετρική διαφορά: 0m"]
["","","","","(5) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]