{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RXM50N2V1B","FFA60A2VEB9 / RXM60N2V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","5.00"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","772"]
["","EER","","","3.24"]
["","COP","","","3.49"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A"]
["","","Θέρμανση","","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","5.80"]
["Σημειώσεις","","","","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσωτερική θερμοκρασία: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσ. θερμοκρ.: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m"]
["","","","","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Outdoor unit","","","","","RXM60N2V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","","5.70"]
["Απόδοση θέρμανσης","Ονομ.","","kW","","7.00"]
["Ονομαστική απόδοση","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","","934"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","","B"]
["","","Θέρμανση","","","B"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","","A+"]
["","Απόδοση","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","347"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","","A+"]
["","Απόδοση","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Pdh Θερμαντική απόδοση στους -10°","","kW","","3.66"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","1372"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","A+++ ~ D"]