{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB9","FFA35A2VEB9","FFA50A2VEB9","FFA60A2VEB9"]
["Περίβλημα","Υλικό","","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","260","260","260","260"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","575","575","575","575"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","575","575","575","575"]
["Βάρος","Μονάδα","","","kg","16.0","16.0","17.5","17.5"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","9.0","10.0","12.7","14.5"]
["","","","Μέτρια","m³/min","8.0","8.5","10.9","12.5"]
["","","","Χαμηλή","m³/min","6.5","6.5","8.6","9.5"]
["","","Θέρμανση","Υψ.","m³/min","9.0","10.0","12.7","14.5"]
["","","","Μέτρια","m³/min","8.0","8.5","10.9","12.5"]
["","","","Χαμηλή","m³/min","6.5","6.5","8.6","9.5"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","48.0","51.0","56.0","60.0"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","31.0","34.0","39.0","43.0"]
["","","","Μέτρια","dBA","28.5","30.5","34.0","40.0"]
["","","","Χαμηλή","dBA","25.0","25.0","27.0","32.0"]
["","Θέρμανση","","Υψ.","dBA","31.0","34.0","39.0","43.0"]
["","","","Μέτρια","dBA","28.5","30.5","34.0","40.0"]
["","","","Χαμηλή","dBA","25.0","25.0","27.0","32.0"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","6","6","6","6"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","9.52","9.52","12.70","12.70"]
["","Αποχέτευση","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Διακοσμητική μάσκα","Μοντέλο","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Χρώμα","","","","Λευκό (N9.5)","Λευκό (N9.5)","Λευκό (N9.5)","Λευκό (N9.5)"]
["","Διαστάσεις","","Διακοσμητική μάσκα-=-Διαστάσεις-=-Ύψος-=-χιλ.","χιλ.","46","46","46","46"]
["","","","Διακοσμητική μάσκα-=-Διαστάσεις-=-Πλάτος-=-χιλ.","χιλ.","620","620","620","620"]
["","","","Διακοσμητική μάσκα-=-Διαστάσεις-=-Βάθος-=-χιλ.","χιλ.","620","620","620","620"]
["","Βάρος","","","kg","2.8","2.8","2.8","2.8"]
["Διακοσμητική μάσκα 2","Μοντέλο","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Χρώμα","","","","Ασημί","Ασημί","Ασημί","Ασημί"]
["","Διαστάσεις","","Διακοσμητική μάσκα 2-=-Διαστάσεις-=-Ύψος-=-χιλ.","χιλ.","46","46","46","46"]
["","","","Πλάτος","χιλ.","620","620","620","620"]
["","","","Βάθος","χιλ.","620","620","620","620"]
["","Βάρος","","","kg","2.8","2.8","2.8","2.8"]
["Διακοσμητική μάσκα 3","Μοντέλο","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Χρώμα","","","","Λευκό (RAL9010)","Λευκό (RAL9010)","Λευκό (RAL9010)","Λευκό (RAL9010)"]
["","Διαστάσεις","","Ύψος","χιλ.","55","55","55","55"]
["","","","Πλάτος","χιλ.","700","700","700","700"]
["","","","Βάθος","χιλ.","700","700","700","700"]
["","Βάρος","","","kg","2.7","2.7","2.7","2.7"]
["Διακοσμητική μάσκα 4","Μοντέλο","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Χρώμα","","","","Λευκό (RAL9010)","Λευκό (RAL9010)","Λευκό (RAL9010)","Λευκό (RAL9010)"]
["","Διαστάσεις","","Ύψος","χιλ.","55","55","55","55"]
["","","","Πλάτος","χιλ.","700","700","700","700"]
["","","","Βάθος","χιλ.","700","700","700","700"]
["","Βάρος","","","kg","2.7","2.7","2.7","2.7"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","BRC7EB530 (στάνταρ πάνελ), BRC7F530W (λευκό πάνελ), BRC7F530S (γκρι πάνελ)","BRC7EB530 (στάνταρ πάνελ), BRC7F530W (λευκό πάνελ), BRC7F530S (γκρι πάνελ)","BRC7EB530 (στάνταρ πάνελ), BRC7F530W (λευκό πάνελ), BRC7F530S (γκρι πάνελ)","BRC7EB530 (στάνταρ πάνελ), BRC7F530W (λευκό πάνελ), BRC7F530S (γκρι πάνελ)"]
["","Τηλεχειριστήριο με καλώδιο","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Στάνταρτ εξαρτήματα","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240"]