{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXM-A8"]
[]
[]
[]
[]
["","","","","FHA50AVEB98 / RXM50A5V1B8"]
["Απόδοση ψύξης","Ονομ.","","kW","5"]
["Απόδοση θέρμανσης","Ονομ.","","kW","6"]
["Ονομαστική απόδοση","EER","","","3.1"]
["","COP","","","3.23"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","806"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","B"]
["","","Θέρμανση","","C"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A+"]
["","Απόδοση","Pdesign","kW","5"]
["","SEER","","","5.84"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","300"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A"]
["","Απόδοση","Pdesign","kW","4.35"]
["","SCOP/A","","","3.82"]
["","Pdh Θερμαντική απόδοση στους -10°","","kW","3.55"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","1594"]
["Σημειώσεις","","","","(1) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","(2) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσ. θερμοκρ.: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m"]
["","","","","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]