{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","36","37","37","38"]
["","","Ονομ.","dBA","34","35","35","36"]
["","","Μέτρια","dBA","31","32","33","34"]
["","Ψύξη","Μέτρια","dBA","34","35","35","36"]
["","","Χαμηλή","dBA","31","32","33","34"]
["","","Υψ.","dBA","36","37","37","38"]
["Στάνταρτ εξαρτήματα","Θερμομονωτικός σωλήνας","","","2","2","2","2"]
["","Υλικό σφικτήρα καλωδίου","","","7","7","7","7"]
["","Ταινία εύκαμπτου σωλήνα","","","1","1","1","1"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","1","1","1","1"]
["","Ροδέλα","","","8","8","8","8"]
["","Στεγανοποιητικό παρέμβυσμα (μεγάλο)","","","1","1","1","1"]
["","Στεγανοποιητικό παρέμβυσμα (μικρό)","","","1","1","1","1"]
["","Τριβικός δακτύλιος ρητίνης","","","1","1","1","1"]
["","Κοχλίες","","","2","2","2","2"]
["","Διάταξη συνδεσμολογίας","","","2","2","2","2"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Piping connections","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","9.52"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","9.50","12.7","12.7","15.9"]
["","Συμπυκνωμάτων","","","VP20","VP20","VP20","VP20"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","53","54","54","55"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","960","960","1,270","1,270"]
["","","Βάθος","mm","690","690","690","690"]
["","","Ύψος","mm","235","235","235","235"]
["Περίβλημα","Υλικό","","","Ρητίνη, λαμαρίνα","Ρητίνη, λαμαρίνα","Ρητίνη, λαμαρίνα","Ρητίνη, λαμαρίνα"]
["","Colour","","","Λευκό","Λευκό","Λευκό","Λευκό"]
["Βάρος","Μονάδα","","kg","24.0","25.0","31.0","32.0"]
["Power supply","Φάση","","","1~","1~","1~","1~"]
["","Συχνότητα","","Hz","50","50","50","50"]
["","Τάση","","V","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]