{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXS-K"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / RXS35K2V1B","FHQ50CAVEB / RXS50K2V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","3.4","5.0"]
["Απόδοση θέρμανσης","Ονομ.","","kW","4","6.0"]
["Ονομαστική απόδοση","EER","","","3.58","3.18"]
["","COP","","","3.96","3.35"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","475","785"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","B"]
["","","Θέρμανση","","A","C"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","B","A"]
["","Απόδοση","Pdesign","kW","3.40","5.00"]
["","SEER","","","4.89","5.48"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","243","320"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A","A"]
["","Απόδοση","Pdesign","kW","3.10","4.35"]
["","SCOP/A","","","3.98","3.74"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","1090.75","1627.83"]