{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":23,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ100CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG71L8Y1B","FHQ71CBVEB / RZQG71L8Y1B","FHQ100CBVEB / RZQG100L8Y1B","FHQ140CBVEB / RZQG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG125L8Y1B","FHQ125CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG125L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG125L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG125L8Y1B","FHQ60CBVEB / FHQ60CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG140L7Y1B"]
["Ψύξη χώρου","SEER","","","6.95","5.10","5.10","5.10","6.86","6.11","6.11","5.10","5.10","5.10","5.10","5.10","5.10","6.01","6.01","5.10","5.10","5.10"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","343","467","467","467","347","545","545","652","652","652","652","652","824","699","699","824","824","824"]
["","Απόδοση","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","B","B","B","A++","A++","A++","B","B","B","B","B","B","A+","A+","B","B","B"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","7.60","6.00","6.00","6.00","7.60","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.71","14.13","14.13","12.71","12.71","12.71"]
["","SCOP/A","","","4.32","3.80","3.80","3.80","4.32","4.61","4.61","3.80","3.80","3.80","3.80","3.80","3.80","4.23","4.23","3.80","3.80","3.80"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A+","A","A","A","A+","A++","A++","A","A","A","A","A","A","A+","A+","A","A","A"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","2,463","2,211","2,211","2,211","2,463","3,432","3,432","4,164","4,164","4,164","4,164","4,164","4,683","4,677","4,677","4,683","4,683","4,683"]
["Απόδοση ψύξης","Ονομ.","","kW","","","","","6.8","9.5","","","","","","","","12.0","","","","","13.4"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","","","","","890","1,245","","","","","","","","1,790","","","","","2,025"]
["","EER","","","","","","","3.82","3.81","","","","","","","","3.35","","","","","3.31"]
["","COP","","","","","","","4.13","4.15","","","","","","","","3.89","","","","","3.63"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","","","","","A","A","","","","","","","","A","","","","","A"]
["","","Θέρμανση","","","","","","A","A","","","","","","","","A","","","","","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","","","","","7.5","10.8","","","","","","","","13.5","","","","","15.5"]
["Σημειώσεις","","","","","","","","(1) - Η ετήσια κατανάλωση ενέργειας είναι σύμφωνη με την Οδηγία για την Ενεργειακή Σήμανση 2002/31/EC","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","","","","","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","","","","","(2) - Τα SEER και SCOP είναι σύμφωνα με το EN 14825","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","","","","","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]