{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","46"]
["","","Αθόρυβη λειτουργία","dBA","30"]
["","","Χαμηλή","dBA","33"]
["","Ψύξη","Αθόρυβη λειτουργία","dBA","29"]
["","","Χαμηλή","dBA","32"]
["","","Υψ.","dBA","38"]
["","","Ονομ.","dBA","36"]
["","Ψύξη","Ονομ.","dBA","35"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","1"]
["","Εγχειρίδιο χειρισμού","","","1"]
["","Τηλεχειριστήριο υπερύθρων","","","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","2"]
["","Υποδοχή τηλεχειριστηρίου","","","1"]
["","Πλάκα στήριξης","","","1"]
["","Θερμομονωτικός σωλήνας (σωλήνας ψυκτικού)","","","8"]
["","Φίλτρο καθαρισμού αέρα","","","1"]
["","Φωτοκαταλυτικό αποσμητικό φίλτρο","","","1"]
["","Πλαϊνό κάλυμμα","","","2"]
["","Ταινία πρόσδεσης","","","4"]
["Control systems","Infrared remote control","","","ARC433B67"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","9.5"]
["","Drain","","","18"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","53"]
["","Θέρμανση","","dBA","59"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","1,050"]
["","","Βάθος","mm","200"]
["","","Ύψος","mm","490"]
["Casing","Χρώμα","","","Κοκαλί"]
["Βάρος","Μονάδα","","kg","16"]
["Power supply","Φάση","","","1~"]
["","Συχνότητα","","Hz","50"]
["","Όνομα","","","VM"]
["","Τάση","","V","220-240"]
["Σημειώσεις","","","","(1) - 220V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]
["","","","","(4) - Κατά τη σύνδεση με σύστημα εξωτερικής μονάδας multi, ανατρέξτε στις προδιαγραφές του συστήματος multi που πρόκειται να συνδεθεί."]