{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A"]
[]
[]
[]
[]
["","","","","FNQ25A2VEB","FNQ35A2VEB","FNQ50A2VEB","FNQ60A2VEB"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","33","33","36","36"]
["","","Ονομ.","dBA","31","31","33","33"]
["","","Χαμηλή","dBA","28","28","30","30"]
["","Ψύξη","Χαμηλή","dBA","28","28","30","30"]
["","","Υψ.","dBA","33","33","36","36"]
["","","Ονομ.","dBA","31","31","33","33"]
["Ψυκτικό μέσο","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Συστήματα ελέγχου","Τηλεχειριστήριο με καλώδιο","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Απόδοση ψύξης","Συνολική απόδοση","Ονομ.","kW","2.6","3.4","5.0","6.0"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","6.35"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52","12.7","12.7"]
["","Συμπυκνωμάτων","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","53","53","56","56"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","790","790","1,190","1,190"]
["","","Βάθος","mm","200","200","200","200"]
["","","Ύψος","mm","620, 720 (2)","620, 720 (2)","620, 720 (2)","620, 720 (2)"]
["Περίβλημα","Υλικό","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["","Χρώμα","","","Άβαφο","Άβαφο","Άβαφο","Άβαφο"]
["Βάρος","Μονάδα","","kg","23","23","30","30"]
["Ανεμιστήρας","Εξωτερική στατική πίεση","Υψηλή","Pa","48","48","49","49"]
["","","Ονομ.","Pa","30","30","40","40"]
["Απόδοση θέρμανσης","Συνολική απόδοση","Ονομ.","kW","3.2","4.0","5.8","7.0"]
["Power supply","Φάση","","","1~","1~","1~","1~"]
["","Συχνότητα","","Hz","50/60","50/60","50/60","50/60"]
["","Τάση","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Σημειώσεις","","","","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]
["","","","","(2) - Συμπεριλαμβανόμενων ποδιών εγκατάστασης","(2) - Συμπεριλαμβανόμενων ποδιών εγκατάστασης","(2) - Συμπεριλαμβανόμενων ποδιών εγκατάστασης","(2) - Συμπεριλαμβανόμενων ποδιών εγκατάστασης"]